Battery voltage: 4024 mV

resetting ...

.

U-Boot 2009.08-lab126 (Apr 23 2014 - 01:01:24)

CPU: Freescale i.MX6 family TO0.0 at 996 MHz

Temperature:   39 C, calibration data 0x59350b5f

mx6sl pll1: 996MHz

mx6sl pll2: 528MHz

mx6sl pll3: 480MHz

mx6sl pll8: 50MHz

ipg clock     : 66000000Hz

ipg per clock : 66000000Hz

uart clock    : 80000000Hz

cspi clock    : 60000000Hz

ahb clock     : 132000000Hz

axi clock   : 198000000Hz

emi_slow clock: 22000000Hz

ddr clock     : 396000000Hz

usdhc1 clock  : 198000000Hz

usdhc2 clock  : 198000000Hz

usdhc3 clock  : 198000000Hz

usdhc4 clock  : 198000000Hz

MMC:  FSL_ESDHC: 0,FSL_ESDHC: 1,FSL_ESDHC: 2

Board: Pinot WFO

Boot Reason: [ POR ]

Boot Device: NAND

Board Id: 02722011429404A2

S/N: 90172201430305TB

I2C:   ready

DRAM:  256 MB

Using default environment

In:    serial

Out:   serial

Err:   serial

Quick Memory Test 0x80000000, 0xfff0000

POST done in 60 ms

BOOTMODE OVERRIDE: DIAGS

Battery voltage: 4028 mV

Hit any key to stop autoboot:  1 ... 0 

## Booting kernel from Legacy Image at 80800000 ...

   Image Name:   Linux-3.0.35-lab126

   Image Type:   ARM Linux Kernel Image (uncompressed)

   Data Size:    2420504 Bytes =  2.3 MB

   Load Address: 80008000

   Entry Point:  80008000

   Verifying Checksum ... OK

   Loading Kernel Image ... OK

OK

Starting kernel ...

[    0.000000] Linux version 3.0.35-lab126 (jenkins-official@sjc10-jbuild10) (collect2: ld returned 1 exit status) #1 Wed Apr 23 16:52:30 PDT 2014
[    0.000000] CPU: ARMv7 Processor [412fc09a] revision 10 (ARMv7), cr=10c53c7d
[    0.000000] CPU: VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] Machine: Freescale i.MX 6SoloLite based Wario Board
[    0.000000] Will try to place printk log at 8fffc000
[    0.000000] Memory policy: ECC disabled, Data cache writeback
[    0.000000] CPU identified as i.MX6SoloLite, silicon rev 1.2
[    0.000000] On node 0 totalpages: 65536
[    0.000000] free_area_init_node: node 0, pgdat c04dcc94, node_mem_map c2000000
[    0.000000]   DMA zone: 64 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 8128 pages, LIFO batch:0
[    0.000000]   Normal zone: 448 pages used for memmap
[    0.000000]   Normal zone: 56896 pages, LIFO batch:15
[    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
[    0.000000] pcpu-alloc: [0] 0 
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 65024
[    0.000000] Kernel command line: rootwait log_pos_goal=0x8fffc000 console=ttymxc0,115200 root=/dev/mmcblk0p2 ro ip=off debug video=mxcepdcfb:E60,bpp=8,x_mem=3M
[    0.000000] Prink buffer will be relocated to physical address: 8fff2000
[    0.000000] log_buf_len: 32768
[    0.000000] early log buf free: 31341(95%)
[    0.000000] PID hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000000] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
[    0.000000] Memory: 256MB = 256MB total
[    0.000000] Memory: 254652k/254652k available, 7492k reserved, 0K highmem
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
[    0.000000]     DMA     : 0xfde00000 - 0xffe00000   (  32 MB)
[    0.000000]     vmalloc : 0xd0800000 - 0xf2000000   ( 536 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)
[    0.000000]     modules : 0xbf000000 - 0xc0000000   (  16 MB)
[    0.000000]       .init : 0xc0008000 - 0xc010b000   (1036 kB)
[    0.000000]       .text : 0xc010b000 - 0xc04aa000   (3708 kB)
[    0.000000]       .data : 0xc04aa000 - 0xc04dd7c0   ( 206 kB)
[    0.000000]        .bss : 0xc04dd7e4 - 0xc0504540   ( 156 kB)
[    0.000000] SLUB: Genslabs=13, HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS:624
[    0.000000] MXC GPIO hardware
[    0.000000] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 178956ms
[    0.000000] arm_max_freq=1GHz
[    0.000000] MXC_Early serial console at MMIO 0x2020000 (options '115200')
[    0.000000] bootconsole [ttymxc0] enabled
[    0.000000] Console: colour dummy device 80x30
[    0.259036] Calibrating delay loop... 1987.37 BogoMIPS (lpj=9936896)
[    0.317362] pid_max: default: 32768 minimum: 301
[    0.322238] Mount-cache hash table entries: 512
[    0.327145] CPU: Testing write buffer coherency: ok
[    0.332173] hw perfevents: enabled with ARMv7 Cortex-A9 PMU driver, 7 counters available
[    0.347139] print_constraints: dummy: 
[    0.351089] NET: Registered protocol family 16
[    0.359336] print_constraints: vddpu: 725 <--> 1300 mV at 700 mV fast normal 
[    0.366913] print_constraints: vddcore: 725 <--> 1300 mV at 1475 mV fast normal 
[    0.374609] print_constraints: vddsoc: 725 <--> 1300 mV at 1475 mV fast normal 
[    0.382273] print_constraints: vdd2p5: 2000 <--> 2775 mV at 2400 mV fast normal 
[    0.390003] print_constraints: vdd1p1: 800 <--> 1400 mV at 1100 mV fast normal 
[    0.397680] print_constraints: vdd3p0: 2625 <--> 3400 mV at 3000 mV fast normal 
[    0.406588] LAB126 Board id - 02722011429404A2
[    0.415121] hw-breakpoint: found 6 breakpoint and 1 watchpoint registers.
[    0.421962] hw-breakpoint: 1 breakpoint(s) reserved for watchpoint single-step.
[    0.429297] hw-breakpoint: maximum watchpoint size is 4 bytes.
[    0.435168] L310 cache controller enabled
[    0.439193] l2x0: 16 ways, CACHE_ID 0x410000c8, AUX_CTRL 0x02030000, Cache size: 262144 B
[    0.455448] bio: create slab <bio-0> at 0
[    0.463095] max77696> regulator init
[    0.467566] spi_imx imx6q-ecspi.0: probed
[    0.472150] usbcore: registered new interface driver usbfs
[    0.477762] usbcore: registered new interface driver hub
[    0.483268] usbcore: registered new device driver usb
[    0.490408] Reboot Reason - Standard Reporting
[    0.494883] kernel: I max77696-irq:evtrcrd: evt=SFT_PRSTRT: Software Partial Restart
[    0.502646] Reboot Reason - Metric Framework Reporting
[    0.507804] kernel: kernel_metric_generic,counter,event_recorder,ercflags,SFT_PRSTRT,1,
[    0.515826] Reboot Reason - Legacy Metric Reporting
[    0.520718] 
[    0.523812] MAX77696 TOPSYS 1.0.0 Installed
[    0.530636] max77696-gpio max77696-gpio.0: gpio#0 -- -- func-0 in 
[    0.538154] max77696-gpio max77696-gpio.0: gpio#1 -- -- func--1 in 
[    0.545896] max77696-gpio max77696-gpio.0: gpio#3 -- -- func-0 in 
[    0.553948] MAX77696 GPIO Driver 1.0.0 Installed
[    0.559628] buck mode: 4
[    0.562941] buck mode: 4
[    0.566417] print_constraints: max77696_buck1: 900 <--> 1300 mV at 1250 mV fast normal idle standby
[    0.576021] buck mode: 4
[    0.579498] print_constraints: max77696_buck1dvs: 600 <--> 1300 mV at 900 mV fast normal idle standby
[    0.589302] buck mode: 4
[    0.592568] buck mode: 4
[    0.596039] print_constraints: max77696_buck2: 900 <--> 1300 mV at 1200 mV fast normal idle standby
[    0.605643] buck mode: 4
[    0.609117] print_constraints: max77696_buck2dvs: 600 <--> 1300 mV at 900 mV fast normal idle standby
[    0.618905] print_constraints: max77696_buck3: 600 <--> 3387 mV at 1300 mV fast normal idle standby
[    0.628690] buck mode: 4
[    0.631956] buck mode: 4
[    0.635222] print_constraints: max77696_buck4: 1200 mV fast normal idle standby
[    0.643075] buck mode: 4
[    0.646550] print_constraints: max77696_buck5: 600 <--> 3387 mV at 1800 mV fast normal idle standby
[    0.656163] buck mode: 4
[    0.659639] print_constraints: max77696_buck6: 600 <--> 3387 mV at 3200 mV fast normal idle standby
[    0.668747] MAX77696 Buck Regulators Driver 1.0.1 Installed
[    0.675106] print_constraints: max77696_ldo1: 800 <--> 3950 mV at 3300 mV normal idle standby
[    0.684241] print_constraints: max77696_ldo2: 800 <--> 3950 mV at 3000 mV normal idle standby
[    0.693324] print_constraints: max77696_ldo3: 800 <--> 3950 mV at 2500 mV normal idle standby
[    0.702436] print_constraints: max77696_ldo4: 800 <--> 2375 mV at 1800 mV normal idle standby
[    0.711500] print_constraints: max77696_ldo5: 800 <--> 2375 mV at 1800 mV normal idle standby
[    0.720618] print_constraints: max77696_ldo6: 800 <--> 3950 mV at 3200 mV normal idle standby
[    0.729701] print_constraints: max77696_ldo7: 800 <--> 3950 mV at 3200 mV normal idle standby
[    0.738811] print_constraints: max77696_ldo8: 800 <--> 2375 mV at 1100 mV normal idle standby
[    0.747880] print_constraints: max77696_ldo9: 800 <--> 2375 mV at 1100 mV normal idle standby
[    0.757007] print_constraints: max77696_ldo10: 2400 <--> 5550 mV at 5200 mV normal idle standby
[    0.766511] MAX77696 Linear Regulators Driver 1.0.2 Installed
[    0.772875] print_constraints: max77696_lsw1: 
[    0.777696] print_constraints: max77696_lsw2: 
[    0.782455] print_constraints: max77696_lsw3: 
[    0.787195] print_constraints: max77696_lsw4: 
[    0.791701] MAX77696 Load Switches Driver 1.0.0 Installed
[    0.798324] print_constraints: max77696-display: 
[    0.803800] print_constraints: max77696-vcom: 
[    0.808579] print_constraints: max77696-vee: 
[    0.813300] print_constraints: max77696-vneg: 
[    0.818083] print_constraints: max77696-vpos: 
[    0.822843] print_constraints: max77696-vddh: 
[    0.828329] 
[    0.828333] EPD vreg probe complete!
[    0.833969] print_constraints: max77696_vddq: 240 <--> 984 mV at 600 mV 
[    0.840747] MAX77696 LPDDR2 Termination Supply Driver 1.0.1 Installed
[    0.848479] MAX77696 I2C Driver 1.0.0 Installed
[    0.855550] i2c-core: driver [max17135] using legacy suspend method
[    0.861838] i2c-core: driver [max17135] using legacy resume method
[    0.868083] Switching to clocksource mxc_timer1
[    0.883134] NET: Registered protocol family 2
[    0.887594] IP route cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.894692] TCP established hash table entries: 8192 (order: 4, 65536 bytes)
[    0.901866] TCP bind hash table entries: 8192 (order: 3, 32768 bytes)
[    0.908399] TCP: Hash tables configured (established 8192 bind 8192)
[    0.914776] TCP reno registered
[    0.917929] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.923792] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.930415] NET: Registered protocol family 1
[    0.935142] RPC: Registered named UNIX socket transport module.
[    0.941081] RPC: Registered udp transport module.
[    0.945819] RPC: Registered tcp transport module.
[    0.950535] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.961190] etb: probe of etb failed with error -2
[    0.966240] etm: probe of etm.0 failed with error -2
[    0.971474] Static Power Management for Freescale i.MX6
[    0.976738] wait mode is enabled for i.MX6
[    0.981025] cpaddr = d0820000 suspend_iram_base=d081c000
[    0.986414] PM driver module loaded
[    0.990172] IMX usb wakeup probe
[    0.993442] the wakeup pdata is 0xce1387c0
[    0.997883] IMX usb wakeup probe
[    1.001131] the wakeup pdata is 0xce1388c0
[    1.005441] cpu regulator mode:ldo_bypass
[    1.009664] _regulator_get: get() with no identifier
[    1.014657] mx6_cpu_regulator_init: failed to get pu regulator
[    1.020703] i.MXC CPU frequency driver
[    1.037557] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    1.044608] msgmni has been set to 497
[    1.048722] io scheduler noop registered
[    1.052761] io scheduler cfq registered (default)
[    1.057977] MAX77696 Backlight Driver 1.0.0 Installed
[    1.063839] imx-sdma imx-sdma: loaded firmware 1.1
[    1.073216] imx-sdma imx-sdma: initialized
[    1.247491] Serial: IMX driver
...................................................................................................................................................................................................................[    1.379640] console [ttymxc0] enabled, bootconsole disabled
[    1.379640] console [ttymxc0] enabled, bootconsole disabled
[    1.395165] loop: module loaded
[    1.398376] MAX77696 32kHz Oscillator Driver 1.0.0 Installed
[    1.404707] input: max77696-onkey as /devices/platform/imx-i2c.0/i2c-0/0-003c/max77696-onkey.0/input/input0
[    1.417909] MAX77696 ONKEY Driver 1.0.0 Installed
[    1.444031] max77696-rtc max77696-rtc.0: rtc core: registered max77696-rtc.0 as rtc0
[    1.463992] max77696-rtc max77696-rtc.0: rtc core: registered max77696-rtc.1 as rtc1
[    1.493299] MAX77696 RTC Driver 1.0.2 Installed
[    1.498713] snvs_rtc snvs_rtc.0: rtc core: registered snvs_rtc as rtc2
[    1.505445] i2c /dev entries driver
[    1.513331] max77696-battery max77696-battery.0: Voltage alert     3400mV ... 4260mV
[    1.521483] max77696-battery max77696-battery.0: SOC alert         (disabled)
[    1.529532] MAX77696 Fuel Gauge Driver 1.0.0 Installed
[    1.536400] MAX77696 USB Interface Circuit Driver 1.0.0 Installed
[    1.544212] max77696-adc max77696-adc.0: ADC average rate: 32 sample(s)
[    1.550833] max77696-adc max77696-adc.0: ADC delay: 0 nsec
[    1.556337] max77696-adc max77696-adc.0: ADC cur src: 50 uA
[    1.561914] MAX77696 ADC Driver 1.0.1 Installed
[    1.567130] imx2-wdt imx2-wdt.0: IMX2+ Watchdog Timer enabled. timeout=60s (nowayout=1)
[    1.575554] sdhci: Secure Digital Host Controller Interface driver
[    1.581738] sdhci: Copyright(c) Pierre Ossman
[    1.586223] mmc0: no vmmc regulator found
[    1.591541] mmc0: SDHCI controller on platform [sdhci-esdhc-imx.1] using DMA
[    1.599676] mmc1: no vmmc regulator found
[    1.606083] mmc1: SDHCI controller on platform [sdhci-esdhc-imx.2] using DMA
[    1.613848] Registered led device: max77696-leds.0
[    1.618648] MAX77696 LED Driver #0 1.0.0 Installed
[    1.627737] Registered led device: max77696-leds.1
[    1.632537] MAX77696 LED Driver #1 1.0.0 Installed
[    1.637868] nf_conntrack version 0.5.0 (3978 buckets, 15912 max)
[    1.646584] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.651959] TCP cubic registered
[    1.655216] NET: Registered protocol family 17
[    1.659676] VFP support v0.3: implementor 41 architecture 3 part 30 variant 9 rev 4
[    1.667484] LPDDR2 MfgId: 0x1 [Samsung]
[    1.671622] Bus freq driver module loaded
[    1.677672] Bus freq driver Enabled
[    1.682158] mxc_dvfs_core_probe
[    1.689751] DVFS driver module loaded
[    1.712861] regulator_init_complete: max77696_ldo10: incomplete constraints, leaving on
[    1.728107] regulator_init_complete: max77696_ldo7: incomplete constraints, leaving on
[    1.745467] regulator_init_complete: max77696_ldo6: incomplete constraints, leaving on
[    1.760673] regulator_init_complete: max77696_buck6: incomplete constraints, leaving on
[    1.768899] regulator_init_complete: max77696_buck5: incomplete constraints, leaving on
[    1.777609] regulator_init_complete: max77696_buck2dvs: incomplete constraints, leaving on
[    1.786314] regulator_init_complete: max77696_buck1dvs: incomplete constraints, leaving on
[    1.795540] emmc: I def:mmcpartinfo:vendor=sandisk, host=mmc0:
[    1.813316] max77696-rtc max77696-rtc.0: setting system clock to 2000-01-01 01:01:07 UTC (946688467)
[    1.842752] mmc0: new high speed DDR MMC card at address 0001
[    1.848903] mmcblk0: mmc0:0001 SEM04G 3.68 GiB 
[    1.853652] mmcblk0boot0: mmc0:0001 SEM04G partition 1 2.00 MiB
[    1.859708] mmcblk0boot1: mmc0:0001 SEM04G partition 2 2.00 MiB
[    1.866674]  mmcblk0: p1 p2 p3 p4
[    1.872873]  mmcblk0boot1: unknown partition table
[    1.879808]  mmcblk0boot0: unknown partition table
[    1.889371] KERNEL: I pmic:charger chgina::charger connected
[    1.900264] MAX77696 Main Charger Driver 1.0.0 Installed
[    1.912874] MAX77696 Energy Harvester Driver 1.0.0 Installed
[    1.919370] Freeing init memory: 1036K
3.0.35-lab126 #1 Wed Apr 23 16:52:30 PDT 2014 armv7l
[    1.949585] INFO:Loaded module /lib/modules/mxc_epdc_eink.ko  (10304 bytes)
[    2.382660] add wake up source irq 104
[    3.522679] KERNEL: I pmic:fg battery id check::wario_battery_valid=1
[    5.209455] INFO:Loaded module /lib/modules/mxc_epdc_fb.ko  (83340 bytes)
[    5.545818] INFO:eink initialized... (786432 bytes)
[    5.550760] INFO:DIAGS MODE
Press [ENTER] for recovery menu...       0 /[    6.560134] INFO:!!! Checking MBR /dev/mmcblk0 !!!!  
[    6.570204] INFO:partition 2, start sector is 782336
[    6.575318] INFO:partition 3, start sector is 913408
[    6.580366] INFO:partition 4, start sector is 1044480
[    6.585503] INFO:maximizing partition 6688768 sectors
[    6.590599] INFO:*** Partition table verified for /dev/mmcblk0 ***
/dev/mmcblk0p4:[    6.600619] INFO:Setup loop device /dev/loop0 for /dev/mmcblk0p4 + 8192

CHS=4/16/104512 size=3424649216 bytes
flag type      first    [    6.611385] INFO:Checking for updates... (auto-pilot mode)
   last  lba first   lba size
Pa[    6.619481] INFO:No update*.bin found; no update needed.
rtition p1:
0x00 0x0b         16 <large>            16    6688752
    CHS: 0/1/1 - <large>
Par[    6.633042] INFO:no updates found.
tition p2:
Partition p3:
Partition p4:
BOOTING DEFAULT.
IP-Config: no devices to configure
[    7.760903] EXT3-fs: barriers not enabled
[    7.765541] kjournald starting.  Commit interval 5 seconds
[    7.771091] EXT3-fs (mmcblk0p2): mounted filesystem with writeback data mode
kinit: Mounted root (ext3 filesystem) readonly.

init started: BusyBox v1.17.1 (2013-09-03 03:06:27 PDT)

starting pid 1138, tty '': '/etc/init.d/rcS'
/etc/init.d/rcS: line 85: boot_milestone: not found
system: I rcS:def:starting /etc/rcS.d/S50diags
USER=root
prevlevel=N
HOME=/
runlevel=S
TERM=vt102
PATH=/sbin:/bin:/usr/sbin:/usr/bin
SHELL=/bin/sh
PWD=/
VERBOSE=no
READ_AHEAD=4
USER=root
prevlevel=N
HOME=/
runlevel=S
TERM=vt102
PATH=/sbin:/bin:/usr/sbin:/usr/bin
SHELL=/bin/sh
PWD=/
VERBOSE=no
IO_SCHED=anticipatory
USER=root
prevlevel=N
HOME=/
runlevel=S
TERM=vt102
PATH=/sbin:/bin:/usr/sbin:/usr/bin
SHELL=/bin/sh
PWD=/
VERBOSE=no
TMP_SIZE=32M
info firsttime:mount_rw:time=7710:Mounting root RW for first boot
[    8.122499] EXT3-fs (mmcblk0p2): using internal journal
info firsttime:cursor:Linking Xorg cursor:
ln: /usr/share/fonts/X11/misc/cursor.pcf: No such file or directory
info firsttime:mount_ro:time=7750:Mounting root RO
[    8.207478] elevator: type 
[    8.207483]  not found
[    8.212659] elevator: switch to 
[    8.212663]  failed
[    8.226517] elevator: type 
[    8.226522]  not found
[    8.231675] elevator: switch to 
[    8.231678]  failed
[    8.245504] elevator: type 
[    8.245509]  not found
[    8.250662] elevator: switch to 
[    8.250666]  failed
info system:start:time=7860:
/etc/rcS.d/S50diags: line 487: f_proto: not found
info hardware:no_wan::WiFi only device. No WAN found
info system:config:platform=wario,board=pinot,rev=34,proto=N,wifi=Y,wan=N:
[    8.305407] udevd (1220): /proc/1220/oom_adj is deprecated, please use /proc/1220/oom_score_adj instead.
info system:done:time=8780:
[    9.196955] ARC USBOTG Device Controller driver (1 August 2005)
[    9.203090] add wake up source irq 75
[    9.211021] USB Cable is already plugged in. Simulating event
[    9.227285] g_file_storage gadget: controller 'fsl-usb2-udc' not recognized
[    9.238523] g_file_storage gadget: File-backed Storage Gadget, version: 1 September 2010
[    9.246659] g_file_storage gadget: Number of LUNs=1
[    9.251548] dr_controller_run: udc out low power mode
[    9.256618] fsl-usb2-udc: bind to driver g_file_storage 
[    9.307325] fuse init (API version 7.16)
[    9.341178] PPP generic driver version 2.4.2
[    9.357775] mwan: I mwan_init:init:wario WAN hardware driver 2.0.0
[    9.364022] mwan: I wan_init:mwan:wan_init
[    9.368354] mwan: D elmo_probe:mwan:elmo_probe::Probing elmo device
[    9.414502] cyttsp4_i2c_adapter 1-0024: cyttsp4_i2c_probe: Starting cyttsp4_i2c_adapter probe...
[    9.423433] cyttsp4_i2c_adapter 1-0024: cyttsp4_i2c_probe: Successful probe cyttsp4_i2c_adapter
[    9.432207] cyttsp4_i2c_init: Cypress TTSP I2C Touchscreen Driver (Built 20121109) rc=0
[    9.450933] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: cyttsp4_core_probe: startup
[    9.459106] g_file_storage gadget: high speed config #1
[    9.468933] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: cyttsp4_core_probe: Init HW
[   10.419572] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: cyttsp4_si_get_test_data: SCANNING is ENABLED codel=0E
[   10.433333] cyttsp4_core:fw:ver=0108:
[   10.441574] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: set_mode: back from wait t=100 cd->mode=4
[   10.472027] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: cyttsp4_startup_: cyttsp4_exit startup r=0...
[   10.481756] cyttsp4_core main_ttsp_core.cyttsp4_i2c_adapter: cyttsp4_core_probe: ok
[   10.542724] cyttsp4_core_init: Cypress TTSP v4 core driver (Built 20121109) rc=0
[   10.556070] cyttsp4_mt cyttsp4_mt.main_ttsp_core: cyttsp4_mt_probe
[   10.584431] input: cyttsp4_mt as /devices/platform/imx-i2c.1/i2c-1/1-0024/main_ttsp_core.cyttsp4_i2c_adapter/cyttsp4_mt.main_ttsp_core/input/input1
[   10.598072] cyttsp4_mt_init: Cypress TTSP MT v4 multi-touch (Built 20121109), rc=0
/etc/rcS.d/S50diags: line 487: iptables-restore: not found
/opt/ar6k/include/dbglog.h.save: No such file or directory
[   10.693832] EXT3-fs: barriers not enabled
[   10.712850] kjournald starting.  Commit interval 5 seconds
[   10.718374] EXT3-fs (mmcblk0p3): warning: mounting fs with errors, running e2fsck is recommended
[   10.744125] EXT3-fs (mmcblk0p3): using internal journal
[   10.749359] EXT3-fs (mmcblk0p3): recovery complete
[   10.755328] EXT3-fs (mmcblk0p3): mounted filesystem with writeback data mode
info userstore:run:time=10400,action=start:
info userstore:found_bootup_flag::Found BOOTUP flag file
dosfsck 2.11 (12 Mar 2005)
dosfsck 2.11, 12 Mar 2005, FAT32, LFN
Checking we can access the last sector of the filesystem
Boot sector contents:
System ID "mkdosfs"
Media byte 0xf8 (hard disk)
       512 bytes per logical sector
      8192 bytes per cluster
      2430 reserved sectors
First FAT starts at byte 1244160 (sector 2430)
         2 FATs, 32 bit entries
   1670656 bytes per FAT (= 3263 sectors)
Root directory start at cluster 2 (arbitrary size)
Data area starts at byte 4585472 (sector 8956)
    417487 data clusters (3420053504 bytes)
32 sectors/track, 64 heads
         0 hidden sectors
   6688752 sectors total
Checking for unused clusters.
Checking free cluster summary.
/dev/loop/0: 1 files, 1/417487 clusters
system: I mntroot:def:Making root filesystem writeable
[   11.472846] EXT3-fs (mmcblk0p2): using internal journal
system: I mntroot:def:Making root filesystem read-only
mounting waveform filesystem
info display:update:Checking '/opt/eink/images/G107_ED060XD4U2' for overrides:
umounting waveform filesystem
drawing default
info display:started:time=11290:
[   17.118185] mmcblk0: error -110 transferring data, sector 878356, nr 2, cmd response 0x900, card status 0xb00
[   17.128125] mmcblk0: retrying using single block read
[   22.557196] mmcblk0: error -110 transferring data, sector 878356, nr 2, cmd response 0x900, card status 0x0
[   22.566967] end_request: I/O error, dev mmcblk0, sector 878356
[   22.573900] mmcblk0: timed out sending r/w cmd command, card status 0x400b00
[   28.004944] mmcblk0: error -110 transferring data, sector 878357, nr 1, cmd response 0x900, card status 0x0
[   28.014716] end_request: I/O error, dev mmcblk0, sector 878357
[   28.020990] EXT3-fs error (device mmcblk0p2): ext3_get_inode_loc: unable to read inode block - inode=1625, block=48010
/etc/rcS.d/S50diags: line 13: /etc/upstart/battery-di[   28.044503] mmc0: Controller never released inhibit bit(s).
[   28.050085] sdhci: =========== REGISTER DUMP (mmc0)===========
[   28.055922] sdhci: Sys addr: 0x00000000 | Version:  0x00000202
[   28.061757] sdhci: Blk size: 0x00000200 | Blk cnt:  0x00000001
[   28.067593] sdhci: Argument: 0x00000002 | Trn mode: 0x00000000
[   28.073428] sdhci: Present:  0xfff98089 | Host ctl: 0x00000021
[   28.079263] sdhci: Power:    0x0000000b | Blk gap:  0x00000000
[   28.085097] sdhci: Wake-up:  0x00000000 | Clock:    0x0000011f
[   28.090932] sdhci: Timeout:  0x00000000 | Int stat: 0x00000000
[   28.096767] sdhci: Int enab: 0x107f00cb | Sig enab: 0x107f00cb
[   28.102601] sdhci: AC12 err: 0x00000000 | Slot int: 0x00000202
[   28.108436] sdhci: Caps:     0x07ebb407 | Caps_1:   0x0000b407
[   28.114271] sdhci: Cmd:      0x0000171a | Max curr: 0x00ffffff
[   28.120105] sdhci: Host ctl2: 0x0000000c
[   28.124028] sdhci: ===========================================
ags: Input/output error
USER=ro[   28.130916] mmcblk0: error -5 sending status command, retrying
ot
prevlevel=N
OLDPWD=/
HOME=/[   28.140822] mmcblk0: timed out sending SET_BLOCK_COUNT command, card status 0x400b00

runlevel=S
TERM=vt102
PATH=/sbin:/bin:/usr/sbin:/usr/bin
SHELL=/bin/sh
PWD=/dev
VERBOSE=no
LD_LIBRARY_PATH=/usr/lib/tts/speech/components/common/:/usr/lib/tts
[   33.575140] mmcblk0: error -110 transferring data, sector 816290, nr 2, cmd response 0x900, card status 0xb00
[   33.585085] mmcblk0: retrying using single block read
[   39.014142] mmcblk0: error -110 transferring data, sector 816290, nr 2, cmd response 0x900, card status 0x0
[   39.023916] end_request: I/O error, dev mmcblk0, sector 816290
[   39.031833] mmcblk0: timed out sending r/w cmd command, card status 0x400b00
[   44.462892] mmcblk0: error -110 transferring data, sector 816291, nr 1, cmd response 0x900, card status 0x0
[   44.472662] end_request: I/O error, dev mmcblk0, sector 816291
[   44.478934] EXT3-fs error (device mmcblk0p2): ext3_find_entry: reading directory #592 offset 0
[   44.497680] mmc0: Controller never released inhibit bit(s).
[   44.503258] sdhci: =========== REGISTER DUMP (mmc0)===========
[   44.509094] sdhci: Sys addr: 0x00000000 | Version:  0x00000202
[   44.514929] sdhci: Blk size: 0x00000200 | Blk cnt:  0x00000001
[   44.520764] sdhci: Argument: 0x00000002 | Trn mode: 0x00000000
[   44.526599] sdhci: Present:  0xfff98089 | Host ctl: 0x00000021
[   44.532434] sdhci: Power:    0x0000000b | Blk gap:  0x00000000
[   44.538269] sdhci: Wake-up:  0x00000000 | Clock:    0x0000011f
[   44.544104] sdhci: Timeout:  0x00000000 | Int stat: 0x00000000
[   44.549939] sdhci: Int enab: 0x107f00cb | Sig enab: 0x107f00cb
[   44.555774] sdhci: AC12 err: 0x00000000 | Slot int: 0x00000202
[   44.561609] sdhci: Caps:     0x07ebb407 | Caps_1:   0x0000b407
[   44.567444] sdhci: Cmd:      0x0000171a | Max curr: 0x00ffffff
[   44.573278] sdhci: Host ctl2: 0x0000000c
[   44.577202] sdhci: ===========================================
[   44.584064] mmcblk0: error -5 sending status command, retrying
[   44.592226] mmcblk0: timed out sending SET_BLOCK_COUNT command, card status 0x400b00
[   50.026008] mmcblk0: error -110 transferring data, sector 816346, nr 2, cmd response 0x900, card status 0xb00
[   50.035948] mmcblk0: retrying using single block read
[   55.464998] mmcblk0: error -110 transferring data, sector 816346, nr 2, cmd response 0x900, card status 0x0
[   55.474768] end_request: I/O error, dev mmcblk0, sector 816346
[   55.482693] mmcblk0: timed out sending r/w cmd command, card status 0x400b00
[   60.913734] mmcblk0: error -110 transferring data, sector 816347, nr 1, cmd response 0x900, card status 0x0
[   60.923501] end_request: I/O error, dev mmcblk0, sector 816347
[   60.929762] EXT3-fs error (device mmcblk0p2): ext3_find_entry: reading directory #592 offset 1
/etc/rcS.d/S50diags: [   60.948956] mmc0: Controller never released inhibit bit(s).
[   60.954535] sdhci: =========== REGISTER DUMP (mmc0)===========
[   60.960372] sdhci: Sys addr: 0x00000000 | Version:  0x00000202
[   60.966207] sdhci: Blk size: 0x00000200 | Blk cnt:  0x00000001
[   60.972042] sdhci: Argument: 0x00000002 | Trn mode: 0x00000000
[   60.977877] sdhci: Present:  0xfff98089 | Host ctl: 0x00000021
[   60.983712] sdhci: Power:    0x0000000b | Blk gap:  0x00000000
[   60.989547] sdhci: Wake-up:  0x00000000 | Clock:    0x0000011f
[   60.995382] sdhci: Timeout:  0x00000000 | Int stat: 0x00000000
[   61.001217] sdhci: Int enab: 0x107f00cb | Sig enab: 0x107f00cb
[   61.007052] sdhci: AC12 err: 0x00000000 | Slot int: 0x00000202
[   61.012887] sdhci: Caps:     0x07ebb407 | Caps_1:   0x0000b407
[   61.018721] sdhci: Cmd:      0x0000171a | Max curr: 0x00ffffff
[   61.024556] sdhci: Host ctl2: 0x0000000c
[   61.028479] sdhci: ===========================================
line 13: kb: not found
[   61.035357] mmcblk0: error -5 sending status command, retrying
[   61.044515] mmcblk0: timed out sending SET_BLOCK_COUNT command, card status 0x400b00
[   66.478295] mmcblk0: error -110 transferring data, sector 782926, nr 2, cmd response 0x900, card status 0xb00
[   66.488232] mmcblk0: retrying using single block read
[   71.917296] mmcblk0: error -110 transferring data, sector 782926, nr 2, cmd response 0x900, card status 0x0
[   71.927083] end_request: I/O error, dev mmcblk0, sector 782926
[   71.934008] mmcblk0: timed out sending r/w cmd command, card status 0x400b00
[   77.365050] mmcblk0: error -110 transferring data, sector 782927, nr 1, cmd response 0x900, card status 0x0
[   77.374830] end_request: I/O error, dev mmcblk0, sector 782927
[   77.381100] EXT3-fs error (device mmcblk0p2): ext3_find_entry: reading directory #34 offset 0
[   77.400151] mmc0: Controller never released inhibit bit(s).
[   77.405730] sdhci: =========== REGISTER DUMP (mmc0)===========
[   77.411566] sdhci: Sys addr: 0x00000000 | Version:  0x00000202
[   77.417402] sdhci: Blk size: 0x00000200 | Blk cnt:  0x00000001
[   77.423238] sdhci: Argument: 0x00000002 | Trn mode: 0x00000000
[   77.429073] sdhci: Present:  0xfff98089 | Host ctl: 0x00000021
[   77.434908] sdhci: Power:    0x0000000b | Blk gap:  0x00000000
[   77.440743] sdhci: Wake-up:  0x00000000 | Clock:    0x0000011f
[   77.446578] sdhci: Timeout:  0x00000000 | Int stat: 0x00000000
[   77.452413] sdhci: Int enab: 0x107f00cb | Sig enab: 0x107f00cb
[   77.458249] sdhci: AC12 err: 0x00000000 | Slot int: 0x00000202
[   77.464083] sdhci: Caps:     0x07ebb407 | Caps_1:   0x0000b407
[   77.469919] sdhci: Cmd:      0x0000171a | Max curr: 0x00ffffff
[   77.475753] sdhci: Host ctl2: 0x0000000c
[   77.479677] sdhci: ===========================================
[   77.486547] mmcblk0: error -5 sending status command, retrying
[   77.494634] mmcblk0: timed out sending SET_BLOCK_COUNT command, card status 0x400b00
[   82.928401] mmcblk0: error -110 transferring data, sector 846390, nr 2, cmd response 0x900, card status 0xb00
[   82.938353] mmcblk0: retrying using single block read
[   88.367410] mmcblk0: error -110 transferring data, sector 846390, nr 2, cmd response 0x900, card status 0x0
[   88.377189] end_request: I/O error, dev mmcblk0, sector 846390
[   88.385112] mmcblk0: timed out sending r/w cmd command, card status 0x400b00
[   93.816165] mmcblk0: error -110 transferring data, sector 846391, nr 1, cmd response 0x900, card status 0x0
[   93.825942] end_request: I/O error, dev mmcblk0, sector 846391
[   93.832275] EXT3-fs error (device mmcblk0p2): ext3_get_inode_loc: