
231117:112148 wpa_supplicant[20332]: wpa_supplicant v2.10
231117:112148 wpa_supplicant[20332]: random: Trying to read entropy from /dev/random
231117:112148 wpa_supplicant[20332]: Successfully initialized wpa_supplicant
231117:112148 wpa_supplicant[20332]: Initializing interface 'wlan0' conf '/etc/wpa_supplicant.conf' driver 'nl80211' ctrl_interface 'N/A' bridge 'N/A'
231117:112148 wpa_supplicant[20332]: Configuration file '/etc/wpa_supplicant.conf' -> '/etc/wpa_supplicant.conf'
231117:112148 wpa_supplicant[20332]: Reading configuration file '/etc/wpa_supplicant.conf'
231117:112148 wpa_supplicant[20332]: device_name='Kindle'
231117:112148 wpa_supplicant[20332]: ctrl_interface='/var/run/wpa_supplicant'
231117:112148 wpa_supplicant[20332]: ap_scan=2
231117:112148 wpa_supplicant[20332]: update_config=0
231117:112148 wpa_supplicant[20332]: sae_pwe=2
231117:112148 wpa_supplicant[20332]: okc=1
231117:112148 wpa_supplicant[20332]: scan_res_valid_for_connect=25
231117:112148 wpa_supplicant[20332]: nl80211: Using driver-based roaming
231117:112148 wpa_supplicant[20332]: nl80211: TDLS supported
231117:112148 wpa_supplicant[20332]: nl80211: TDLS external setup
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:1
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:5
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:2
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:4
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:6
231117:112148 wpa_supplicant[20332]: nl80211: Supported cipher 00-0f-ac:7
231117:112148 wpa_supplicant[20332]: nl80211: Using driver-based off-channel TX
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=1
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=6
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=4
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1374 subcmd=105
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1374 subcmd=9
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=8
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=10
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=11
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=4354
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=4608
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=7
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=5632
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=5633
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=5121
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=2
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=12
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1374 subcmd=103
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1a11 subcmd=5122
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1374 subcmd=54
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor command: vendor_id=0x1374 subcmd=55
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=0
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=1
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=2
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=3
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=4
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=5
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=6
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1a11 subcmd=7
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0xce7 subcmd=8
231117:112148 wpa_supplicant[20332]: nl80211: Supported vendor event: vendor_id=0x1374 subcmd=54
231117:112148 wpa_supplicant[20332]: nl80211: Use separate P2P group interface (driver advertised support)
231117:112148 wpa_supplicant[20332]: nl80211: Enable multi-channel concurrent (driver advertised support)
231117:112148 wpa_supplicant[20332]: nl80211: key_mgmt=0xd0f enc=0x110f auth=0x7 flags=0x9a9cfac0 rrm_flags=0x0 probe_resp_offloads=0x0 max_stations=16 max_remain_on_chan=5000 max_scan_ssids=11
231117:112148 wpa_supplicant[20332]: nl80211: interface wlan0 in phy phy0
231117:112148 wpa_supplicant[20332]: nl80211: Set mode ifindex 38 iftype 2 (STATION)
231117:112148 wpa_supplicant[20332]: nl80211: Subscribe to mgmt frames with non-AP handle 0x7acaf0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xb0 (WLAN_FC_STYPE_AUTH) nl_handle=0x7acaf0 match=0300 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0801 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=06 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a07 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a11 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1101 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1102 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0505 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0500 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1301 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1305 multicast=0
231117:112148 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=7e506f9a1a multicast=0
231117:112148 wpa_supplicant[20332]: rfkill: Cannot open RFKILL control device
231117:112148 wpa_supplicant[20332]: nl80211: RFKILL status not available
231117:112148 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=1 (userspace-control), operstate=5 (IF_OPER_DORMANT)
231117:112148 wpa_supplicant[20332]: Add interface wlan0 to a new radio phy0
231117:112148 wpa_supplicant[20332]: nl80211: Regulatory information - country=IT (DFS-ETSI)
231117:112148 wpa_supplicant[20332]: nl80211: 2402-2482 @ 40 MHz 20 mBm
231117:112148 wpa_supplicant[20332]: nl80211: 5170-5250 @ 80 MHz 20 mBm
231117:112148 wpa_supplicant[20332]: nl80211: 5250-5330 @ 80 MHz 20 mBm (DFS)
231117:112148 wpa_supplicant[20332]: nl80211: 5490-5710 @ 160 MHz 27 mBm (DFS)
231117:112148 wpa_supplicant[20332]: nl80211: 57000-66000 @ 2160 MHz 40 mBm
231117:112148 wpa_supplicant[20332]: nl80211: Added 802.11b mode based on 802.11g information
231117:112148 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11g: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467[NO_IR] 2472[NO_IR] 2484[DISABLED]
231117:112148 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11a: 5180 5200 5220 5240 5260[NO_IR][RADAR] 5280[NO_IR][RADAR] 5300[NO_IR][RADAR] 5320[NO_IR][RADAR] 5500[NO_IR][RADAR] 5520[NO_IR][RADAR] 5540[NO_IR][RADAR] 5560[NO_IR][RADAR] 5580[NO_IR][RADAR]
231117:112148 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11b: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467[NO_IR] 2472[NO_IR] 2484[DISABLED]
231117:112148 wpa_supplicant[20332]: wlan0: Own MAC address: 08:xx:xx:xx:1b:7d
231117:112148 wpa_supplicant[20332]: Note: nl80211 driver interface is not designed to be used with ap_scan=2; this can result in connection failures
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=0 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=1 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=2 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=3 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=4 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=5 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112148 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112148 wpa_supplicant[20332]:    broadcast key
231117:112148 wpa_supplicant[20332]: wlan0: RSN: flushing PMKID list in the driver
231117:112148 wpa_supplicant[20332]: nl80211: Flush PMKIDs
231117:112148 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> INACTIVE
231117:112148 wpa_supplicant[20332]: wlan0: WPS: UUID based on MAC address: ed8daac7-239b-5ebc-b8ec-611631526934
231117:112148 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state DISCONNECTED
231117:112148 wpa_supplicant[20332]: EAPOL: Supplicant port status: Unauthorized
231117:112148 wpa_supplicant[20332]: nl80211: Skip set_supp_port(unauthorized) while not associated
231117:112148 wpa_supplicant[20332]: EAPOL: KEY_RX entering state NO_KEY_RECEIVE
231117:112148 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state INITIALIZE
231117:112148 wpa_supplicant[20332]: EAP: EAP entering state DISABLED
231117:112148 wpa_supplicant[20332]: wlan0: Added interface wlan0
231117:112148 wpa_supplicant[20332]: wlan0: State: INACTIVE -> DISCONNECTED
231117:112148 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112148 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112148 wpa_supplicant[20332]: random: Got 20/20 bytes from /dev/random
231117:112149 wpa_supplicant[20332]: CTRL_IFACE monitor attached /tmp/wpa_ctrl_1633-44\x00
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'LIST_NETWORKS'
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'STA_AUTOCONNECT 0'
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'ADD_NETWORK'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: ADD_NETWORK
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='group'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=5): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='key_mgmt'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=7): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='pairwise'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='priority'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=2): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='psk'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=12): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='ssid'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=12): [REMOVED]
231117:112149 wpa_supplicant[20332]: nl80211: Drv Event 33 (NL80211_CMD_TRIGGER_SCAN) received for wlan0
231117:112149 wpa_supplicant[20332]: wlan0: nl80211: Scan trigger
231117:112149 wpa_supplicant[20332]: wlan0: Event SCAN_STARTED (47) received
231117:112149 wpa_supplicant[20332]: wlan0: External program started a scan
231117:112149 wpa_supplicant[20332]: nl80211: Drv Event 34 (NL80211_CMD_NEW_SCAN_RESULTS) received for wlan0
231117:112149 wpa_supplicant[20332]: wlan0: nl80211: New scan results available
231117:112149 wpa_supplicant[20332]: nl80211: Scan probed for SSID ''
231117:112149 wpa_supplicant[20332]: nl80211: Scan included frequencies: 2427
231117:112149 wpa_supplicant[20332]: wlan0: Event SCAN_RESULTS (3) received
231117:112149 wpa_supplicant[20332]: nl80211: Received scan results (3 BSSes)
231117:112149 wpa_supplicant[20332]: wlan0: BSS: Start scan result update 1
231117:112149 wpa_supplicant[20332]: wlan0: BSS: Add new id 0 BSSID 3e:xx:xx:xx:ee:80 SSID 'B********i' freq 2427
231117:112149 wpa_supplicant[20332]: wlan0: BSS: Add new id 1 BSSID 38:xx:xx:xx:a1:e2 SSID 'B********i' freq 2427
231117:112149 wpa_supplicant[20332]: wlan0: BSS: Add new id 2 BSSID 3e:xx:xx:xx:ee:c8 SSID 'B********i' freq 2427
231117:112149 wpa_supplicant[20332]: BSS: last_scan_res_used=3/32
231117:112149 wpa_supplicant[20332]: wlan0: New scan results available (own=0 ext=1)
231117:112149 wpa_supplicant[20332]: wlan0: Do not use results from externally requested scan operation for network selection
231117:112149 wpa_supplicant[20332]: EAPOL: disable timer tick
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='pairwise'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='group'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'ENABLE_NETWORK 0'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: ENABLE_NETWORK id=0
231117:112149 wpa_supplicant[20332]: wlan0: Selecting BSS from priority group 42
231117:112149 wpa_supplicant[20332]: wlan0: 0: 3e:xx:xx:xx:ee:80 ssid='B********i' wpa_ie_len=0 rsn_ie_len=20 caps=0x1431 level=-25 freq=2427  wps
231117:112149 wpa_supplicant[20332]: wlan0:    selected based on RSN IE
231117:112149 wpa_supplicant[20332]: wlan0:    selected BSS 3e:xx:xx:xx:ee:80 ssid='B********i'
231117:112149 wpa_supplicant[20332]: wlan0: Considering connect request: reassociate: 1  selected: 3e:xx:xx:xx:ee:80  bssid: 00:xx:xx:xx:00:00  pending: 00:xx:xx:xx:00:00  wpa_state: DISCONNECTED  ssid=0x7c1230  current_ssid=(nil)
231117:112149 wpa_supplicant[20332]: wlan0: Request association with 3e:xx:xx:xx:ee:80
231117:112149 wpa_supplicant[20332]: SAE: Derive PT - group 19
231117:112149 wpa_supplicant[20332]: SAE: SSID - hexdump(len=10): 42 61 69 6f 63 63 68 69 6e 69
231117:112149 wpa_supplicant[20332]: SAE: password - hexdump(len=10): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-seed - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u1 P1) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u1 - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u2 P2) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u2 - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: Derive PT - group 20
231117:112149 wpa_supplicant[20332]: SAE: SSID - hexdump(len=10): 42 61 69 6f 63 63 68 69 6e 69
231117:112149 wpa_supplicant[20332]: SAE: password - hexdump(len=10): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-seed - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u1 P1) - hexdump(len=72): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u1 - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u2 P2) - hexdump(len=72): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u2 - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=48): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: Derive PT - group 21
231117:112149 wpa_supplicant[20332]: SAE: SSID - hexdump(len=10): 42 61 69 6f 63 63 68 69 6e 69
231117:112149 wpa_supplicant[20332]: SAE: password - hexdump(len=10): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-seed - hexdump(len=64): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u1 P1) - hexdump(len=99): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u1 - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: pwd-value (u2 P2) - hexdump(len=99): [REMOVED]
231117:112149 wpa_supplicant[20332]: SAE: u2 - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: m - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: t - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1a = b / (z * a) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1b = (-b/a) * (1 + t) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x1 = CSEL(l, x1a, x1b) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1 = x1^3 + a * x1 + b - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x2 = z * u^2 * x1 - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx2 = x2^3 + a * x2 + b - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: gx1^((p-1)/2) modulo p - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: v = CSEL(l, gx1, gx2) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: x = CSEL(l, x1, x2) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: y = sqrt(v) - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: p - y - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.x - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: SSWU: P.y - hexdump(len=66): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: No ongoing scan/p2p-scan found to abort
231117:112149 wpa_supplicant[20332]: wlan0: Add radio work 'connect'@0x7c3f20
231117:112149 wpa_supplicant[20332]: wlan0: First radio work item in the queue - schedule start immediately
231117:112149 wpa_supplicant[20332]: wlan0: Starting radio work 'connect'@0x7c3f20 after 0.000215 second wait
231117:112149 wpa_supplicant[20332]: wlan0: WPA: clearing own WPA/RSN IE
231117:112149 wpa_supplicant[20332]: wlan0: RSN: clearing own RSNXE
231117:112149 wpa_supplicant[20332]: RSN: PMKSA cache search - network_ctx=0x7c1230 try_opportunistic=1 akmp=0x0
231117:112149 wpa_supplicant[20332]: RSN: Search for BSSID 3e:xx:xx:xx:ee:80
231117:112149 wpa_supplicant[20332]: RSN: Consider 3e:xx:xx:xx:ee:80 for OKC
231117:112149 wpa_supplicant[20332]: RSN: No PMKSA cache entry found
231117:112149 wpa_supplicant[20332]: wlan0: RSN: using IEEE 802.11i/D9.0
231117:112149 wpa_supplicant[20332]: wlan0: WPA: Selected cipher suites: group 16 pairwise 16 key_mgmt 2 proto 2
231117:112149 wpa_supplicant[20332]: wlan0: WPA: Selected mgmt group cipher 32
231117:112149 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112149 wpa_supplicant[20332]: WPA: set AP RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112149 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112149 wpa_supplicant[20332]: wlan0: WPA: AP group 0x10 network profile group 0x10; available group 0x10
231117:112149 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112149 wpa_supplicant[20332]: wlan0: WPA: AP pairwise 0x10 network profile pairwise 0x10; available pairwise 0x10
231117:112149 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112149 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network profile key_mgmt 0x2; available key_mgmt 0x2
231117:112149 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA-PSK
231117:112149 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network profile mgmt_group_cipher 0x0; available mgmt_group_cipher 0x0
231117:112149 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112149 wpa_supplicant[20332]: WPA: Set own WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112149 wpa_supplicant[20332]: RSN: Set own RSNXE default - hexdump(len=0):
231117:112149 wpa_supplicant[20332]: WPA: Set PMK based on external data - hexdump(len=32): [REMOVED]
231117:112149 wpa_supplicant[20332]: wlan0: Automatic auth_alg selection: 0x1
231117:112149 wpa_supplicant[20332]: Added supported operating classes IE - hexdump(len=20): 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112149 wpa_supplicant[20332]: wlan0: Trying to associate with SSID 'B********i'
231117:112149 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112149 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> ASSOCIATING
231117:112149 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112149 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112149 wpa_supplicant[20332]: nl80211: Set mode ifindex 38 iftype 2 (STATION)
231117:112149 wpa_supplicant[20332]: nl80211: Unsubscribe mgmt frames handle 0x88f24279 (mode change)
231117:112149 wpa_supplicant[20332]: nl80211: Subscribe to mgmt frames with non-AP handle 0x7acaf0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xb0 (WLAN_FC_STYPE_AUTH) nl_handle=0x7acaf0 match=0300 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0801 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=06 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a07 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a11 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1101 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1102 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0505 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0500 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1301 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1305 multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=7e506f9a1a multicast=0
231117:112149 wpa_supplicant[20332]: nl80211: Connect (ifindex=38)
231117:112149 wpa_supplicant[20332]:   * bssid_hint=3e:xx:xx:xx:ee:80
231117:112149 wpa_supplicant[20332]:   * freq_hint=2427
231117:112149 wpa_supplicant[20332]:   * SSID=B********i
231117:112149 wpa_supplicant[20332]:   * IEs - hexdump(len=55): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 7f 0b 00 00 00 00 00 00 40 00 00 00 20 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112149 wpa_supplicant[20332]:   * WPA Versions 0x2
231117:112149 wpa_supplicant[20332]:   * pairwise=0xfac04
231117:112149 wpa_supplicant[20332]:   * group=0xfac04
231117:112149 wpa_supplicant[20332]:   * akm=0xfac02
231117:112149 wpa_supplicant[20332]:   * Auth Type 0
231117:112149 wpa_supplicant[20332]: nl80211: Connect request send successfully
231117:112149 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 60 sec 0 usec
231117:112149 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112149 wpa_supplicant[20332]: EAPOL: External notification - EAP fail=0
231117:112149 wpa_supplicant[20332]: EAPOL: External notification - portControl=Auto
231117:112149 wpa_supplicant[20332]: wlan0: Control interface command 'SELECT_NETWORK 0'
231117:112149 wpa_supplicant[20332]: CTRL_IFACE: SELECT_NETWORK id=0
231117:112149 wpa_supplicant[20332]: Already associated with the selected network - do nothing
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 46 (NL80211_CMD_CONNECT) received for wlan0
231117:112150 wpa_supplicant[20332]: nl80211: Connect event (status=0 ignore_next_local_disconnect=0)
231117:112150 wpa_supplicant[20332]: nl80211: Associated on 2427 MHz
231117:112150 wpa_supplicant[20332]: nl80211: Associated with 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: nl80211: Operating frequency for the associated BSS from scan results: 2427 MHz
231117:112150 wpa_supplicant[20332]: nl80211: Associated on 2427 MHz
231117:112150 wpa_supplicant[20332]: nl80211: Associated with 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: nl80211: Set drv->ssid based on scan res info to 'B********i'
231117:112150 wpa_supplicant[20332]: wlan0: Event ASSOC (0) received
231117:112150 wpa_supplicant[20332]: wlan0: Association info event
231117:112150 wpa_supplicant[20332]: req_ies - hexdump(len=156): 00 0a 42 61 69 6f 63 63 68 69 6e 69 01 08 02 04 0b 16 0c 12 18 24 32 04 30 48 60 6c 21 02 0a 14 24 0a 01 0d 24 04 34 04 64 0c 95 05 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82 2d 1a 3d 01 03 ff 00 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 7f 08 00 00 00 00 00 00 01 41 bf 0c 30 01 80 03 fe ff 00 00 fe ff 00 00 dd 07 00 50 f2 02 00 01 00 dd 07 00 0c e7 08 00 00 00
231117:112150 wpa_supplicant[20332]: resp_ies - hexdump(len=274): 01 08 82 84 8b 0c 12 96 18 24 32 04 30 48 60 6c 46 05 73 d0 00 00 0c 2d 1a ad 09 03 ff ff 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 3d 16 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 4a 0e 14 00 0a 00 2c 01 c8 00 14 00 05 00 19 00 7f 08 04 00 0f 02 00 00 00 40 bf 0c 92 39 89 33 fe ff 00 00 fa ff 00 20 c0 05 00 04 00 fc ff ff 02 27 03 ff 0e 26 00 08 a9 ff 2f a9 ff 45 75 ff 65 75 ff dd 17 8c fd f0 01 01 02 01 00 02 01 01 03 03 01 01 00 04 01 01 09 02 00 00 dd 1f 8c fd f0 00 00 01 03 00 ff 00 00 3e 94 ed 48 a1 e2 a8 00 38 94 ed 48 ee 82 3e 94 ed 48 ee 80 dd 18 00 50 f2 02 01 01 80 00 03 a4 00 00 27 a4 00 00 42 43 5e 00 62 32 2f 00 dd 07 8c fd f0 04 01 01 00 dd 0b 00 14 6c 00 07 0f 00 00 8e 1c 96 dd 18 00 50 f2 04 10 4a 00 01 10 10 3b 00 01 03 10 49 00 06 00 37 2a 00 01 20
231117:112150 wpa_supplicant[20332]: wlan0: freq=2427 MHz
231117:112150 wpa_supplicant[20332]: WPA: set own WPA/RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: wlan0: RSN: clearing own RSNXE
231117:112150 wpa_supplicant[20332]: wlan0: State: ASSOCIATING -> ASSOCIATED
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112150 wpa_supplicant[20332]: wlan0: Associated to a new BSS: BSSID=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: Select network based on association information
231117:112150 wpa_supplicant[20332]: wlan0: Network configuration found for the current AP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Using WPA IE from AssocReq to set cipher suites
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected cipher suites: group 16 pairwise 16 key_mgmt 2 proto 2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected mgmt group cipher 32
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSN IE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP group 0x10 network profile group 0x10; available group 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP pairwise 0x10 network profile pairwise 0x10; available pairwise 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network profile key_mgmt 0x2; available key_mgmt 0x2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA-PSK
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network profile mgmt_group_cipher 0x0; available mgmt_group_cipher 0x0
231117:112150 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112150 wpa_supplicant[20332]: WPA: Set own WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: WPA: Leave previously set WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: RSN: Set own RSNXE default - hexdump(len=0):
231117:112150 wpa_supplicant[20332]: WPA: Set PMK based on external data - hexdump(len=32): [REMOVED]
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP fail=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portControl=Auto
231117:112150 wpa_supplicant[20332]: WPA: Update cipher suite selection based on IEs in driver-generated WPA/RSNE in AssocReq - hexdump(len=112): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82 2d 1a 3d 01 03 ff 00 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 7f 08 00 00 00 00 00 00 01 41 bf 0c 30 01 80 03 fe ff 00 00 fe ff 00 00 dd 07 00 50 f2 02 00 01 00 dd 07 00 0c e7 08 00 00 00
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network key_mgmt 0x2; available key_mgmt 0x2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA2-PSK and proto 2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP pairwise cipher 0x10 network pairwise cipher 0x10; available pairwise cipher 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP group cipher 0x10 network group cipher 0x10; available group cipher 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network mgmt_group_cipher 0x0; available mgmt_group_cipher 0x20
231117:112150 wpa_supplicant[20332]: wlan0: WPA: STA/AP is not MFP capable; AP RSNE caps 0xc
231117:112150 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112150 wpa_supplicant[20332]: wlan0: Associated with 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Association event - clear replay counter
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Clear old PTK
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=1
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state CONNECTING
231117:112150 wpa_supplicant[20332]: EAPOL: enable timer tick
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state IDLE
231117:112150 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 10 sec 0 usec
231117:112150 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-SUBNET-STATUS-UPDATE status=0
231117:112150 wpa_supplicant[20332]: l2_packet_receive: src=3e:xx:xx:xx:ee:80 len=99
231117:112150 wpa_supplicant[20332]: wlan0: RX EAPOL from 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 10 sec 0 usec
231117:112150 wpa_supplicant[20332]: wlan0: IEEE 802.1X RX: version=2 type=3 length=95
231117:112150 wpa_supplicant[20332]: wlan0:   EAPOL-Key type=2
231117:112150 wpa_supplicant[20332]: wlan0:   key_info 0x8a (ver=2 keyidx=0 rsvd=0 Pairwise Ack)
231117:112150 wpa_supplicant[20332]: wlan0:   key_length=16 key_data_length=0
231117:112150 wpa_supplicant[20332]:   replay_counter - hexdump(len=8): 00 00 00 00 00 00 00 01
231117:112150 wpa_supplicant[20332]:   key_nonce - hexdump(len=32): 79 be 4c 7e 73 7e dd 55 cc d2 1c 7c d0 0e 3d a4 87 42 41 60 64 94 0f 5f ec 1a 17 e5 7a 65 61 01
231117:112150 wpa_supplicant[20332]:   key_iv - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_rsc - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_id (reserved) - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_mic - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]: wlan0: State: ASSOCIATED -> 4WAY_HANDSHAKE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: RX message 1 of 4-Way Handshake from 3e:xx:xx:xx:ee:80 (ver=2)
231117:112150 wpa_supplicant[20332]: RSN: msg 1/4 key data - hexdump(len=0):
231117:112150 wpa_supplicant[20332]: WPA: Renewed SNonce - hexdump(len=32): 37 ca 62 a3 6b 04 0c 8c 6b 7b 37 dd 85 e3 1a 5f 82 fb 5b a0 05 e6 f7 17 97 d2 11 b5 b0 bb 5c f8
231117:112150 wpa_supplicant[20332]: WPA: PTK derivation using PRF(SHA1)
231117:112150 wpa_supplicant[20332]: WPA: PTK derivation - A1=08:xx:xx:xx:1b:7d A2=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: WPA: Nonce1 - hexdump(len=32): 37 ca 62 a3 6b 04 0c 8c 6b 7b 37 dd 85 e3 1a 5f 82 fb 5b a0 05 e6 f7 17 97 d2 11 b5 b0 bb 5c f8
231117:112150 wpa_supplicant[20332]: WPA: Nonce2 - hexdump(len=32): 79 be 4c 7e 73 7e dd 55 cc d2 1c 7c d0 0e 3d a4 87 42 41 60 64 94 0f 5f ec 1a 17 e5 7a 65 61 01
231117:112150 wpa_supplicant[20332]: WPA: PMK - hexdump(len=32): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: PTK - hexdump(len=48): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: KEK - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: TK - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: WPA IE for msg 2/4 - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: WPA: Replay Counter - hexdump(len=8): 00 00 00 00 00 00 00 01
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Sending EAPOL-Key 2/4
231117:112150 wpa_supplicant[20332]: WPA: Send EAPOL-Key frame to 3e:xx:xx:xx:ee:80 ver=2 mic_len=16 key_mgmt=0x2
231117:112150 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112150 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: Derived Key MIC - hexdump(len=16): 6c e7 69 60 2b d8 57 ba a1 ce c6 7c 03 8c 21 27
231117:112150 wpa_supplicant[20332]: l2_packet_receive: src=3e:xx:xx:xx:ee:80 len=155
231117:112150 wpa_supplicant[20332]: wlan0: RX EAPOL from 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: IEEE 802.1X RX: version=2 type=3 length=151
231117:112150 wpa_supplicant[20332]: wlan0:   EAPOL-Key type=2
231117:112150 wpa_supplicant[20332]: wlan0:   key_info 0x13ca (ver=2 keyidx=0 rsvd=0 Pairwise Install Ack MIC Secure Encr)
231117:112150 wpa_supplicant[20332]: wlan0:   key_length=16 key_data_length=56
231117:112150 wpa_supplicant[20332]:   replay_counter - hexdump(len=8): 00 00 00 00 00 00 00 02
231117:112150 wpa_supplicant[20332]:   key_nonce - hexdump(len=32): 79 be 4c 7e 73 7e dd 55 cc d2 1c 7c d0 0e 3d a4 87 42 41 60 64 94 0f 5f ec 1a 17 e5 7a 65 61 01
231117:112150 wpa_supplicant[20332]:   key_iv - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_rsc - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_id (reserved) - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:   key_mic - hexdump(len=16): 8e 33 e6 ba 74 18 5c 74 92 ad 58 e8 fc f2 0f 4f
231117:112150 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112150 wpa_supplicant[20332]: RSN: encrypted key data - hexdump(len=56): d0 9a 1d ec 8a 8f e4 cd 59 65 d6 59 97 26 bb 75 b1 83 02 d2 a9 d6 bc 25 1a 75 01 35 3f 7c 55 c1 6b 2b 26 90 74 ad ea fc e3 f8 3d 58 77 9f f4 4c 06 b7 69 62 b0 04 9d 8a
231117:112150 wpa_supplicant[20332]: WPA: Decrypt Key Data using AES-UNWRAP (KEK length 16)
231117:112150 wpa_supplicant[20332]: WPA: decrypted EAPOL-Key key data - hexdump(len=48): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: State: 4WAY_HANDSHAKE -> 4WAY_HANDSHAKE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: RX message 3 of 4-Way Handshake from 3e:xx:xx:xx:ee:80 (ver=2)
231117:112150 wpa_supplicant[20332]: WPA: IE KeyData - hexdump(len=48): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00 dd 16 00 0f ac 01 01 00 10 7a ff b6 84 74 d9 e2 37 43 f0 dd 2b 67 6e ef dd 00
231117:112150 wpa_supplicant[20332]: WPA: RSN IE in EAPOL-Key - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112150 wpa_supplicant[20332]: WPA: GTK in EAPOL-Key - hexdump(len=24): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: WPA: No WPA/RSN IE for this AP known. Trying to get from scan results
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112150 wpa_supplicant[20332]: WPA: set AP RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Found the current AP from updated scan results
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Sending EAPOL-Key 4/4
231117:112150 wpa_supplicant[20332]: WPA: Send EAPOL-Key frame to 3e:xx:xx:xx:ee:80 ver=2 mic_len=16 key_mgmt=0x2
231117:112150 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112150 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: Derived Key MIC - hexdump(len=16): f9 14 83 63 3a 75 77 7e 37 e2 43 95 bd f2 64 d2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Installing PTK to the driver
231117:112150 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=3 addr=0x7ad04c key_idx=0 set_tx=1 seq_len=6 key_len=16 key_flag=0x2c
231117:112150 wpa_supplicant[20332]: nl80211: NEW_KEY
231117:112150 wpa_supplicant[20332]: nl80211: KEY_DATA - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: nl80211: KEY_SEQ - hexdump(len=6): 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:    addr=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]:    pairwise key
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portValid=1
231117:112150 wpa_supplicant[20332]: wlan0: State: 4WAY_HANDSHAKE -> GROUP_HANDSHAKE
231117:112150 wpa_supplicant[20332]: RSN: received GTK in pairwise handshake - hexdump(len=18): [REMOVED]
231117:112150 wpa_supplicant[20332]: WPA: Group Key - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Installing GTK to the driver (keyidx=1 tx=0 len=16)
231117:112150 wpa_supplicant[20332]: WPA: RSC - hexdump(len=6): 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=3 addr=0xa5f5b key_idx=1 set_tx=0 seq_len=6 key_len=16 key_flag=0x14
231117:112150 wpa_supplicant[20332]: nl80211: NEW_KEY
231117:112150 wpa_supplicant[20332]: nl80211: KEY_DATA - hexdump(len=16): [REMOVED]
231117:112150 wpa_supplicant[20332]: nl80211: KEY_SEQ - hexdump(len=6): 00 00 00 00 00 00
231117:112150 wpa_supplicant[20332]:    broadcast key
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Key negotiation completed with 3e:xx:xx:xx:ee:80 [PTK=CCMP GTK=CCMP]
231117:112150 wpa_supplicant[20332]: wlan0: Cancelling authentication timeout
231117:112150 wpa_supplicant[20332]: wlan0: State: GROUP_HANDSHAKE -> COMPLETED
231117:112150 wpa_supplicant[20332]: wlan0: Radio work 'connect'@0x7c3f20 done in 0.348081 seconds
231117:112150 wpa_supplicant[20332]: wlan0: radio_work_free('connect'@0x7c3f20): num_active_works --> 0
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-CONNECTED - Connection to 3e:xx:xx:xx:ee:80 completed [id=0 id_str= freq=2427]
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->1 (UP)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=6 (IF_OPER_UP)
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portValid=1
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=1
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state AUTHENTICATING
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state SUCCESS
231117:112150 wpa_supplicant[20332]: EAP: EAP entering state DISABLED
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state AUTHENTICATED
231117:112150 wpa_supplicant[20332]: EAPOL: Supplicant port status: Authorized
231117:112150 wpa_supplicant[20332]: nl80211: Set supplicant port authorized for 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state IDLE
231117:112150 wpa_supplicant[20332]: EAPOL authentication completed - result=SUCCESS
231117:112150 wpa_supplicant[20332]: nl80211: Set rekey offload
231117:112150 wpa_supplicant[20332]: EAPOL: EAP Session-Id not available
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 48 (NL80211_CMD_DISCONNECT) received for wlan0
231117:112150 wpa_supplicant[20332]: nl80211: Disconnect event
231117:112150 wpa_supplicant[20332]: wlan0: Event DEAUTH (11) received
231117:112150 wpa_supplicant[20332]: wlan0: Deauthentication notification
231117:112150 wpa_supplicant[20332]: wlan0:  * reason 1 (UNSPECIFIED)
231117:112150 wpa_supplicant[20332]: Deauthentication frame IE(s) - hexdump(len=0): [NULL]
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-DISCONNECTED bssid=3e:xx:xx:xx:ee:80 reason=1
231117:112150 wpa_supplicant[20332]: wlan0: Auto connect disabled: do not try to re-connect
231117:112150 wpa_supplicant[20332]: wlan0: Ignore connection failure indication since interface has been put into disconnected state
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Clear old PMK and PTK
231117:112150 wpa_supplicant[20332]: wlan0: Disconnect event - remove keys
231117:112150 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=0 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112150 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112150 wpa_supplicant[20332]:    broadcast key
231117:112150 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=1 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112150 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112150 wpa_supplicant[20332]:    broadcast key
231117:112150 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=0x7ab3ec key_idx=0 set_tx=0 seq_len=0 key_len=0 key_flag=0x20
231117:112150 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112150 wpa_supplicant[20332]:    addr=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]:    pairwise key
231117:112150 wpa_supplicant[20332]: wlan0: State: COMPLETED -> DISCONNECTED
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 1->0 (DORMANT)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state DISCONNECTED
231117:112150 wpa_supplicant[20332]: EAPOL: Supplicant port status: Unauthorized
231117:112150 wpa_supplicant[20332]: nl80211: Skip set_supp_port(unauthorized) while not associated
231117:112150 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state INITIALIZE
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 36 (NL80211_CMD_REG_CHANGE) received for wlan0
231117:112150 wpa_supplicant[20332]: nl80211: Regulatory domain change
231117:112150 wpa_supplicant[20332]:  * initiator=0
231117:112150 wpa_supplicant[20332]:  * type=1
231117:112150 wpa_supplicant[20332]: wlan0: Event CHANNEL_LIST_CHANGED (27) received
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-REGDOM-CHANGE init=CORE type=WORLD
231117:112150 wpa_supplicant[20332]: wlan0: Updating hw mode
231117:112150 wpa_supplicant[20332]: nl80211: Regulatory information - country=IT (DFS-ETSI)
231117:112150 wpa_supplicant[20332]: nl80211: 2402-2482 @ 40 MHz 20 mBm
231117:112150 wpa_supplicant[20332]: nl80211: 5170-5250 @ 80 MHz 20 mBm
231117:112150 wpa_supplicant[20332]: nl80211: 5250-5330 @ 80 MHz 20 mBm (DFS)
231117:112150 wpa_supplicant[20332]: nl80211: 5490-5710 @ 160 MHz 27 mBm (DFS)
231117:112150 wpa_supplicant[20332]: nl80211: 57000-66000 @ 2160 MHz 40 mBm
231117:112150 wpa_supplicant[20332]: nl80211: Added 802.11b mode based on 802.11g information
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11g: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11a: 5180 5200 5220 5240 5260[NO_IR][RADAR] 5280[NO_IR][RADAR] 5300[NO_IR][RADAR] 5320[NO_IR][RADAR] 5500[NO_IR][RADAR] 5520[NO_IR][RADAR] 5540[NO_IR][RADAR] 5560[NO_IR][RADAR] 5580[NO_IR][RADAR]
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11b: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 36 (NL80211_CMD_REG_CHANGE) received for wlan0
231117:112150 wpa_supplicant[20332]: nl80211: Regulatory domain change
231117:112150 wpa_supplicant[20332]:  * initiator=1
231117:112150 wpa_supplicant[20332]:  * type=0
231117:112150 wpa_supplicant[20332]:  * alpha2=IT
231117:112150 wpa_supplicant[20332]: wlan0: Event CHANNEL_LIST_CHANGED (27) received
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-REGDOM-CHANGE init=USER type=COUNTRY alpha2=IT
231117:112150 wpa_supplicant[20332]: wlan0: Updating hw mode
231117:112150 wpa_supplicant[20332]: nl80211: Regulatory information - country=IT (DFS-ETSI)
231117:112150 wpa_supplicant[20332]: nl80211: 2402-2482 @ 40 MHz 20 mBm
231117:112150 wpa_supplicant[20332]: nl80211: 5170-5250 @ 80 MHz 20 mBm
231117:112150 wpa_supplicant[20332]: nl80211: 5250-5330 @ 80 MHz 20 mBm (DFS)
231117:112150 wpa_supplicant[20332]: nl80211: 5490-5710 @ 160 MHz 27 mBm (DFS)
231117:112150 wpa_supplicant[20332]: nl80211: 57000-66000 @ 2160 MHz 40 mBm
231117:112150 wpa_supplicant[20332]: nl80211: Added 802.11b mode based on 802.11g information
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11g: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11a: 5180 5200 5220 5240 5260[NO_IR][RADAR] 5280[NO_IR][RADAR] 5300[NO_IR][RADAR] 5320[NO_IR][RADAR] 5500[NO_IR][RADAR] 5520[NO_IR][RADAR] 5540[NO_IR][RADAR] 5560[NO_IR][RADAR] 5580[NO_IR][RADAR]
231117:112150 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11b: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 33 (NL80211_CMD_TRIGGER_SCAN) received for wlan0
231117:112150 wpa_supplicant[20332]: wlan0: nl80211: Scan trigger
231117:112150 wpa_supplicant[20332]: wlan0: Event SCAN_STARTED (47) received
231117:112150 wpa_supplicant[20332]: wlan0: External program started a scan
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='pairwise'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='group'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'ENABLE_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: ENABLE_NETWORK id=0
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SELECT_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SELECT_NETWORK id=0
231117:112150 wpa_supplicant[20332]: wlan0: Scan results matching the currently selected network
231117:112150 wpa_supplicant[20332]: wlan0: 0: 3e:xx:xx:xx:ee:80 freq=2427 level=-25 snr=64 est_throughput=65000
231117:112150 wpa_supplicant[20332]: wlan0: 1: 38:xx:xx:xx:a1:e2 freq=2427 level=-57 snr=32 est_throughput=65000
231117:112150 wpa_supplicant[20332]: wlan0: 2: 3e:xx:xx:xx:ee:c8 freq=2427 level=-70 snr=19 est_throughput=55250
231117:112150 wpa_supplicant[20332]: wlan0: Selecting BSS from priority group 42
231117:112150 wpa_supplicant[20332]: wlan0: 0: 3e:xx:xx:xx:ee:80 ssid='B********i' wpa_ie_len=0 rsn_ie_len=20 caps=0x1431 level=-25 freq=2427  wps
231117:112150 wpa_supplicant[20332]: wlan0:    selected based on RSN IE
231117:112150 wpa_supplicant[20332]: wlan0:    selected BSS 3e:xx:xx:xx:ee:80 ssid='B********i'
231117:112150 wpa_supplicant[20332]: wlan0: Considering connect request: reassociate: 1  selected: 3e:xx:xx:xx:ee:80  bssid: 00:xx:xx:xx:00:00  pending: 00:xx:xx:xx:00:00  wpa_state: DISCONNECTED  ssid=0x7c1230  current_ssid=0x7c1230
231117:112150 wpa_supplicant[20332]: wlan0: Request association with 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: Re-association to the same ESS
231117:112150 wpa_supplicant[20332]: wlan0: No ongoing scan/p2p-scan found to abort
231117:112150 wpa_supplicant[20332]: wlan0: Add radio work 'connect'@0x7c4788
231117:112150 wpa_supplicant[20332]: wlan0: First radio work item in the queue - schedule start immediately
231117:112150 wpa_supplicant[20332]: Delay radio work start until externally triggered scan completes
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 34 (NL80211_CMD_NEW_SCAN_RESULTS) received for wlan0
231117:112150 wpa_supplicant[20332]: wlan0: nl80211: New scan results available
231117:112150 wpa_supplicant[20332]: nl80211: Scan probed for SSID ''
231117:112150 wpa_supplicant[20332]: nl80211: Scan included frequencies: 2427
231117:112150 wpa_supplicant[20332]: wlan0: Event SCAN_RESULTS (3) received
231117:112150 wpa_supplicant[20332]: nl80211: Received scan results (5 BSSes)
231117:112150 wpa_supplicant[20332]: wlan0: BSS: Start scan result update 2
231117:112150 wpa_supplicant[20332]: wlan0: BSS: Add new id 3 BSSID 38:xx:xx:xx:ee:80 SSID '' freq 2427
231117:112150 wpa_supplicant[20332]: wlan0: BSS: Add new id 4 BSSID 3e:xx:xx:xx:a1:e2 SSID '' freq 2427
231117:112150 wpa_supplicant[20332]: BSS: last_scan_res_used=5/32
231117:112150 wpa_supplicant[20332]: wlan0: New scan results available (own=0 ext=1)
231117:112150 wpa_supplicant[20332]: wlan0: Do not use results from externally requested scan operation for network selection
231117:112150 wpa_supplicant[20332]: wlan0: Starting radio work 'connect'@0x7c4788 after 0.035148 second wait
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing own WPA/RSN IE
231117:112150 wpa_supplicant[20332]: wlan0: RSN: clearing own RSNXE
231117:112150 wpa_supplicant[20332]: RSN: PMKSA cache search - network_ctx=0x7c1230 try_opportunistic=1 akmp=0x0
231117:112150 wpa_supplicant[20332]: RSN: Search for BSSID 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: RSN: Consider 3e:xx:xx:xx:ee:80 for OKC
231117:112150 wpa_supplicant[20332]: RSN: No PMKSA cache entry found
231117:112150 wpa_supplicant[20332]: wlan0: RSN: using IEEE 802.11i/D9.0
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected cipher suites: group 16 pairwise 16 key_mgmt 2 proto 2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected mgmt group cipher 32
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112150 wpa_supplicant[20332]: WPA: set AP RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP group 0x10 network profile group 0x10; available group 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP pairwise 0x10 network profile pairwise 0x10; available pairwise 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network profile key_mgmt 0x2; available key_mgmt 0x2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA-PSK
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network profile mgmt_group_cipher 0x0; available mgmt_group_cipher 0x0
231117:112150 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112150 wpa_supplicant[20332]: WPA: Set own WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: RSN: Set own RSNXE default - hexdump(len=0):
231117:112150 wpa_supplicant[20332]: WPA: Set PMK based on external data - hexdump(len=32): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Automatic auth_alg selection: 0x1
231117:112150 wpa_supplicant[20332]: Added supported operating classes IE - hexdump(len=20): 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112150 wpa_supplicant[20332]: wlan0: Trying to associate with SSID 'B********i'
231117:112150 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112150 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> ASSOCIATING
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112150 wpa_supplicant[20332]: nl80211: Set mode ifindex 38 iftype 2 (STATION)
231117:112150 wpa_supplicant[20332]: nl80211: Unsubscribe mgmt frames handle 0x88f24279 (mode change)
231117:112150 wpa_supplicant[20332]: nl80211: Subscribe to mgmt frames with non-AP handle 0x7acaf0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xb0 (WLAN_FC_STYPE_AUTH) nl_handle=0x7acaf0 match=0300 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0801 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=06 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a07 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a11 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1101 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1102 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0505 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0500 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1301 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1305 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=7e506f9a1a multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Connect (ifindex=38)
231117:112150 wpa_supplicant[20332]:   * bssid_hint=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]:   * freq_hint=2427
231117:112150 wpa_supplicant[20332]:   * SSID=B********i
231117:112150 wpa_supplicant[20332]:   * IEs - hexdump(len=55): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 7f 0b 00 00 00 00 00 00 40 00 00 00 20 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112150 wpa_supplicant[20332]:   * WPA Versions 0x2
231117:112150 wpa_supplicant[20332]:   * pairwise=0xfac04
231117:112150 wpa_supplicant[20332]:   * group=0xfac04
231117:112150 wpa_supplicant[20332]:   * akm=0xfac02
231117:112150 wpa_supplicant[20332]:   * Auth Type 0
231117:112150 wpa_supplicant[20332]: nl80211: Connect request send successfully
231117:112150 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 60 sec 0 usec
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP fail=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portControl=Auto
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='pairwise'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='group'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'ENABLE_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: ENABLE_NETWORK id=0
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SELECT_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SELECT_NETWORK id=0
231117:112150 wpa_supplicant[20332]: Already associated with the selected network - do nothing
231117:112150 wpa_supplicant[20332]: nl80211: Drv Event 46 (NL80211_CMD_CONNECT) received for wlan0
231117:112150 wpa_supplicant[20332]: nl80211: Connect event (status=37 ignore_next_local_disconnect=0)
231117:112150 wpa_supplicant[20332]: wlan0: Event ASSOC_REJECT (12) received
231117:112150 wpa_supplicant[20332]: wlan0: CTRL-EVENT-ASSOC-REJECT bssid=3e:xx:xx:xx:ee:80 status_code=37
231117:112150 wpa_supplicant[20332]: wlan0: Radio work 'connect'@0x7c4788 done in 0.250095 seconds
231117:112150 wpa_supplicant[20332]: wlan0: radio_work_free('connect'@0x7c4788): num_active_works --> 0
231117:112150 wpa_supplicant[20332]: Added BSSID 3e:xx:xx:xx:ee:80 into ignore list, ignoring for 10 seconds
231117:112150 wpa_supplicant[20332]: wlan0: Consecutive connection failures: 1 --> request scan in 100 ms
231117:112150 wpa_supplicant[20332]: wlan0: Setting scan request: 0.100000 sec
231117:112150 wpa_supplicant[20332]: wlan0: State: ASSOCIATING -> DISCONNECTED
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='priority'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=2): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='pairwise'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='group'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=4): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'ENABLE_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: ENABLE_NETWORK id=0
231117:112150 wpa_supplicant[20332]: wlan0: Control interface command 'SELECT_NETWORK 0'
231117:112150 wpa_supplicant[20332]: CTRL_IFACE: SELECT_NETWORK id=0
231117:112150 wpa_supplicant[20332]: wlan0: Scan results matching the currently selected network
231117:112150 wpa_supplicant[20332]: Removed BSSID 3e:xx:xx:xx:ee:80 from ignore list (clear)
231117:112150 wpa_supplicant[20332]: wlan0: 0: 3e:xx:xx:xx:ee:80 freq=2427 level=-25 snr=64 est_throughput=65000
231117:112150 wpa_supplicant[20332]: wlan0: 2: 38:xx:xx:xx:a1:e2 freq=2427 level=-55 snr=34 est_throughput=65000
231117:112150 wpa_supplicant[20332]: wlan0: 4: 3e:xx:xx:xx:ee:c8 freq=2427 level=-70 snr=19 est_throughput=55250
231117:112150 wpa_supplicant[20332]: wlan0: Selecting BSS from priority group 41
231117:112150 wpa_supplicant[20332]: wlan0: 0: 3e:xx:xx:xx:ee:80 ssid='B********i' wpa_ie_len=0 rsn_ie_len=20 caps=0x1431 level=-25 freq=2427  wps
231117:112150 wpa_supplicant[20332]: wlan0:    selected based on RSN IE
231117:112150 wpa_supplicant[20332]: wlan0:    selected BSS 3e:xx:xx:xx:ee:80 ssid='B********i'
231117:112150 wpa_supplicant[20332]: wlan0: Considering connect request: reassociate: 1  selected: 3e:xx:xx:xx:ee:80  bssid: 00:xx:xx:xx:00:00  pending: 00:xx:xx:xx:00:00  wpa_state: DISCONNECTED  ssid=0x7c1230  current_ssid=0x7c1230
231117:112150 wpa_supplicant[20332]: wlan0: Request association with 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: wlan0: Re-association to the same ESS
231117:112150 wpa_supplicant[20332]: wlan0: No ongoing scan/p2p-scan found to abort
231117:112150 wpa_supplicant[20332]: wlan0: Add radio work 'connect'@0x7c3f90
231117:112150 wpa_supplicant[20332]: wlan0: First radio work item in the queue - schedule start immediately
231117:112150 wpa_supplicant[20332]: wlan0: Starting radio work 'connect'@0x7c3f90 after 0.000220 second wait
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing own WPA/RSN IE
231117:112150 wpa_supplicant[20332]: wlan0: RSN: clearing own RSNXE
231117:112150 wpa_supplicant[20332]: RSN: PMKSA cache search - network_ctx=0x7c1230 try_opportunistic=1 akmp=0x0
231117:112150 wpa_supplicant[20332]: RSN: Search for BSSID 3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]: RSN: Consider 3e:xx:xx:xx:ee:80 for OKC
231117:112150 wpa_supplicant[20332]: RSN: No PMKSA cache entry found
231117:112150 wpa_supplicant[20332]: wlan0: RSN: using IEEE 802.11i/D9.0
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected cipher suites: group 16 pairwise 16 key_mgmt 2 proto 2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: Selected mgmt group cipher 32
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112150 wpa_supplicant[20332]: WPA: set AP RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112150 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP group 0x10 network profile group 0x10; available group 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP pairwise 0x10 network profile pairwise 0x10; available pairwise 0x10
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network profile key_mgmt 0x2; available key_mgmt 0x2
231117:112150 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA-PSK
231117:112150 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network profile mgmt_group_cipher 0x0; available mgmt_group_cipher 0x0
231117:112150 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112150 wpa_supplicant[20332]: WPA: Set own WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112150 wpa_supplicant[20332]: RSN: Set own RSNXE default - hexdump(len=0):
231117:112150 wpa_supplicant[20332]: WPA: Set PMK based on external data - hexdump(len=32): [REMOVED]
231117:112150 wpa_supplicant[20332]: wlan0: Automatic auth_alg selection: 0x1
231117:112150 wpa_supplicant[20332]: Added supported operating classes IE - hexdump(len=20): 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112150 wpa_supplicant[20332]: wlan0: Trying to associate with SSID 'B********i'
231117:112150 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112150 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> ASSOCIATING
231117:112150 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112150 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112150 wpa_supplicant[20332]: nl80211: Set mode ifindex 38 iftype 2 (STATION)
231117:112150 wpa_supplicant[20332]: nl80211: Unsubscribe mgmt frames handle 0x88f24279 (mode change)
231117:112150 wpa_supplicant[20332]: nl80211: Subscribe to mgmt frames with non-AP handle 0x7acaf0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xb0 (WLAN_FC_STYPE_AUTH) nl_handle=0x7acaf0 match=0300 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0801 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=06 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a07 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0a11 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1101 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1102 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0505 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=0500 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1301 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=1305 multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Register frame type=0xd0 (WLAN_FC_STYPE_ACTION) nl_handle=0x7acaf0 match=7e506f9a1a multicast=0
231117:112150 wpa_supplicant[20332]: nl80211: Connect (ifindex=38)
231117:112150 wpa_supplicant[20332]:   * bssid_hint=3e:xx:xx:xx:ee:80
231117:112150 wpa_supplicant[20332]:   * freq_hint=2427
231117:112150 wpa_supplicant[20332]:   * SSID=B********i
231117:112150 wpa_supplicant[20332]:   * IEs - hexdump(len=55): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 7f 0b 00 00 00 00 00 00 40 00 00 00 20 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82
231117:112150 wpa_supplicant[20332]:   * WPA Versions 0x2
231117:112150 wpa_supplicant[20332]:   * pairwise=0xfac04
231117:112150 wpa_supplicant[20332]:   * group=0xfac04
231117:112150 wpa_supplicant[20332]:   * akm=0xfac02
231117:112150 wpa_supplicant[20332]:   * Auth Type 0
231117:112150 wpa_supplicant[20332]: nl80211: Connect request send successfully
231117:112150 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 60 sec 0 usec
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - EAP fail=0
231117:112150 wpa_supplicant[20332]: EAPOL: External notification - portControl=Auto
231117:112152 wpa_supplicant[20332]: EAPOL: startWhen --> 0
231117:112152 wpa_supplicant[20332]: EAPOL: disable timer tick
231117:112153 wpa_supplicant[20332]: nl80211: Drv Event 46 (NL80211_CMD_CONNECT) received for wlan0
231117:112153 wpa_supplicant[20332]: nl80211: Connect event (status=0 ignore_next_local_disconnect=0)
231117:112153 wpa_supplicant[20332]: nl80211: Associated on 5200 MHz
231117:112153 wpa_supplicant[20332]: nl80211: Associated with 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: nl80211: Operating frequency for the associated BSS from scan results: 5200 MHz
231117:112153 wpa_supplicant[20332]: nl80211: Associated on 5200 MHz
231117:112153 wpa_supplicant[20332]: nl80211: Associated with 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: nl80211: Set drv->ssid based on scan res info to 'B********i'
231117:112153 wpa_supplicant[20332]: wlan0: Event ASSOC (0) received
231117:112153 wpa_supplicant[20332]: wlan0: Association info event
231117:112153 wpa_supplicant[20332]: req_ies - hexdump(len=150): 00 0a 42 61 69 6f 63 63 68 69 6e 69 01 08 0c 12 18 24 30 48 60 6c 21 02 0a 14 24 0a 01 0d 24 04 34 04 64 0b 95 05 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82 2d 1a 7f 11 03 ff 00 00 00 01 00 00 00 00 00 00 00 01 00 00 00 01 00 00 00 00 00 00 7f 08 01 00 00 00 00 00 00 40 bf 0c 30 71 90 03 fe ff 00 00 fe ff 00 00 dd 07 00 50 f2 02 00 01 00 dd 07 00 0c e7 08 00 00 00
231117:112153 wpa_supplicant[20332]: resp_ies - hexdump(len=268): 01 08 8c 12 98 24 b0 48 60 6c 46 05 73 d0 00 00 0c 2d 1a ef 09 03 ff ff 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 3d 16 28 07 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 4a 0e 14 00 0a 00 2c 01 c8 00 14 00 05 00 19 00 7f 08 04 00 0f 02 00 00 00 40 bf 0c b2 39 89 33 fe ff 00 00 fa ff 00 20 c0 05 01 2a 00 fc ff ff 02 27 03 ff 0e 26 01 08 a9 ff 2f a9 ff 45 75 ff 65 75 ff dd 17 8c fd f0 01 01 02 01 00 02 01 01 03 03 01 01 00 04 01 01 09 02 00 00 dd 1f 8c fd f0 00 00 01 03 00 ff 00 00 00 00 00 00 00 00 00 00 38 94 ed 48 ee 81 00 00 00 00 00 00 dd 18 00 50 f2 02 01 01 8f 00 03 a4 00 00 27 a4 00 00 42 43 5e 00 62 32 2f 00 dd 07 8c fd f0 04 01 01 00 dd 0b 00 14 6c 00 07 0f 00 00 8e 1c 96 dd 18 00 50 f2 04 10 4a 00 01 10 10 3b 00 01 03 10 49 00 06 00 37 2a 00 01 20
231117:112153 wpa_supplicant[20332]: wlan0: freq=5200 MHz
231117:112153 wpa_supplicant[20332]: WPA: set own WPA/RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112153 wpa_supplicant[20332]: wlan0: RSN: clearing own RSNXE
231117:112153 wpa_supplicant[20332]: wlan0: State: ASSOCIATING -> ASSOCIATED
231117:112153 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112153 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112153 wpa_supplicant[20332]: wlan0: Associated to a new BSS: BSSID=38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: wlan0: Select network based on association information
231117:112153 wpa_supplicant[20332]: wlan0: Network configuration found for the current AP
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Using WPA IE from AssocReq to set cipher suites
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Selected cipher suites: group 16 pairwise 16 key_mgmt 2 proto 2
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Selected mgmt group cipher 32
231117:112153 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSN IE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP group 0x10 network profile group 0x10; available group 0x10
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP pairwise 0x10 network profile pairwise 0x10; available pairwise 0x10
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network profile key_mgmt 0x2; available key_mgmt 0x2
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA-PSK
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network profile mgmt_group_cipher 0x0; available mgmt_group_cipher 0x0
231117:112153 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112153 wpa_supplicant[20332]: WPA: Set own WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112153 wpa_supplicant[20332]: WPA: Leave previously set WPA IE default - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112153 wpa_supplicant[20332]: RSN: Set own RSNXE default - hexdump(len=0):
231117:112153 wpa_supplicant[20332]: WPA: Set PMK based on external data - hexdump(len=32): [REMOVED]
231117:112153 wpa_supplicant[20332]: nl80211: Received scan results (13 BSSes)
231117:112153 wpa_supplicant[20332]: nl80211: Scan results indicate BSS status with 38:xx:xx:xx:ee:81 as associated
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Start scan result update 3
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 5 BSSID 38:xx:xx:xx:ee:82 SSID '' freq 5540
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 6 BSSID 38:xx:xx:xx:ee:81 SSID 'B********i' freq 5200
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 7 BSSID 14:xx:xx:xx:69:81 SSID 'V****************1' freq 5560
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 8 BSSID 38:xx:xx:xx:a1:e4 SSID '' freq 5540
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 9 BSSID 38:xx:xx:xx:a1:e3 SSID 'B********i' freq 5200
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 10 BSSID 38:xx:xx:xx:ee:ca SSID '' freq 5540
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 11 BSSID 22:xx:xx:xx:77:c9 SSID 'F************1' freq 5280
231117:112153 wpa_supplicant[20332]: wlan0: BSS: Add new id 12 BSSID a6:xx:xx:xx:6e:78 SSID 'T**********9' freq 5220
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - EAP fail=0
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portControl=Auto
231117:112153 wpa_supplicant[20332]: WPA: Update cipher suite selection based on IEs in driver-generated WPA/RSNE in AssocReq - hexdump(len=112): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00 3b 12 51 51 53 54 73 74 75 76 77 78 79 7a 7b 7c 7d 80 81 82 2d 1a 7f 11 03 ff 00 00 00 01 00 00 00 00 00 00 00 01 00 00 00 01 00 00 00 00 00 00 7f 08 01 00 00 00 00 00 00 40 bf 0c 30 71 90 03 fe ff 00 00 fe ff 00 00 dd 07 00 50 f2 02 00 01 00 dd 07 00 0c e7 08 00 00 00
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP key_mgmt 0x2 network key_mgmt 0x2; available key_mgmt 0x2
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using KEY_MGMT WPA2-PSK and proto 2
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP pairwise cipher 0x10 network pairwise cipher 0x10; available pairwise cipher 0x10
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using PTK CCMP
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP group cipher 0x10 network group cipher 0x10; available group cipher 0x10
231117:112153 wpa_supplicant[20332]: wlan0: WPA: using GTK CCMP
231117:112153 wpa_supplicant[20332]: wlan0: WPA: AP mgmt_group_cipher 0x20 network mgmt_group_cipher 0x0; available mgmt_group_cipher 0x20
231117:112153 wpa_supplicant[20332]: wlan0: WPA: STA/AP is not MFP capable; AP RSNE caps 0xc
231117:112153 wpa_supplicant[20332]: wlan0: WPA: not using MGMT group cipher
231117:112153 wpa_supplicant[20332]: wlan0: Associated with 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Association event - clear replay counter
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Clear old PTK
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=1
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state CONNECTING
231117:112153 wpa_supplicant[20332]: EAPOL: enable timer tick
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state IDLE
231117:112153 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 10 sec 0 usec
231117:112153 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112153 wpa_supplicant[20332]: wlan0: CTRL-EVENT-SUBNET-STATUS-UPDATE status=0
231117:112153 wpa_supplicant[20332]: l2_packet_receive: src=38:xx:xx:xx:ee:81 len=99
231117:112153 wpa_supplicant[20332]: wlan0: RX EAPOL from 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: wlan0: Setting authentication timeout: 10 sec 0 usec
231117:112153 wpa_supplicant[20332]: wlan0: IEEE 802.1X RX: version=2 type=3 length=95
231117:112153 wpa_supplicant[20332]: wlan0:   EAPOL-Key type=2
231117:112153 wpa_supplicant[20332]: wlan0:   key_info 0x8a (ver=2 keyidx=0 rsvd=0 Pairwise Ack)
231117:112153 wpa_supplicant[20332]: wlan0:   key_length=16 key_data_length=0
231117:112153 wpa_supplicant[20332]:   replay_counter - hexdump(len=8): 00 00 00 00 00 00 00 01
231117:112153 wpa_supplicant[20332]:   key_nonce - hexdump(len=32): 2a bb 63 e0 eb d5 36 6e 9f b2 11 25 02 76 ac 12 17 f1 0d d6 9d eb e4 b0 fb d9 10 72 80 ad a1 d0
231117:112153 wpa_supplicant[20332]:   key_iv - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_rsc - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_id (reserved) - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_mic - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]: wlan0: State: ASSOCIATED -> 4WAY_HANDSHAKE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: RX message 1 of 4-Way Handshake from 38:xx:xx:xx:ee:81 (ver=2)
231117:112153 wpa_supplicant[20332]: RSN: msg 1/4 key data - hexdump(len=0):
231117:112153 wpa_supplicant[20332]: WPA: Renewed SNonce - hexdump(len=32): ed c0 08 21 89 2d 76 49 1f 0c b2 e1 1c 84 17 ad 98 cc f8 7a 0b 78 fd 50 a5 88 6d 9c 11 83 be d7
231117:112153 wpa_supplicant[20332]: WPA: PTK derivation using PRF(SHA1)
231117:112153 wpa_supplicant[20332]: WPA: PTK derivation - A1=08:xx:xx:xx:1b:7d A2=38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: WPA: Nonce1 - hexdump(len=32): ed c0 08 21 89 2d 76 49 1f 0c b2 e1 1c 84 17 ad 98 cc f8 7a 0b 78 fd 50 a5 88 6d 9c 11 83 be d7
231117:112153 wpa_supplicant[20332]: WPA: Nonce2 - hexdump(len=32): 2a bb 63 e0 eb d5 36 6e 9f b2 11 25 02 76 ac 12 17 f1 0d d6 9d eb e4 b0 fb d9 10 72 80 ad a1 d0
231117:112153 wpa_supplicant[20332]: WPA: PMK - hexdump(len=32): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: PTK - hexdump(len=48): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: KEK - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: TK - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: WPA IE for msg 2/4 - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 00 00
231117:112153 wpa_supplicant[20332]: WPA: Replay Counter - hexdump(len=8): 00 00 00 00 00 00 00 01
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Sending EAPOL-Key 2/4
231117:112153 wpa_supplicant[20332]: WPA: Send EAPOL-Key frame to 38:xx:xx:xx:ee:81 ver=2 mic_len=16 key_mgmt=0x2
231117:112153 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112153 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: Derived Key MIC - hexdump(len=16): e8 b8 c9 0e 49 9d b0 1c 73 88 ec 9f 7a 6e ba de
231117:112153 wpa_supplicant[20332]: l2_packet_receive: src=38:xx:xx:xx:ee:81 len=155
231117:112153 wpa_supplicant[20332]: wlan0: RX EAPOL from 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: wlan0: IEEE 802.1X RX: version=2 type=3 length=151
231117:112153 wpa_supplicant[20332]: wlan0:   EAPOL-Key type=2
231117:112153 wpa_supplicant[20332]: wlan0:   key_info 0x13ca (ver=2 keyidx=0 rsvd=0 Pairwise Install Ack MIC Secure Encr)
231117:112153 wpa_supplicant[20332]: wlan0:   key_length=16 key_data_length=56
231117:112153 wpa_supplicant[20332]:   replay_counter - hexdump(len=8): 00 00 00 00 00 00 00 02
231117:112153 wpa_supplicant[20332]:   key_nonce - hexdump(len=32): 2a bb 63 e0 eb d5 36 6e 9f b2 11 25 02 76 ac 12 17 f1 0d d6 9d eb e4 b0 fb d9 10 72 80 ad a1 d0
231117:112153 wpa_supplicant[20332]:   key_iv - hexdump(len=16): 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_rsc - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_id (reserved) - hexdump(len=8): 00 00 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:   key_mic - hexdump(len=16): fc 4e 8a 4a 97 35 18 36 61 55 cd 0c 57 56 c8 cc
231117:112153 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112153 wpa_supplicant[20332]: RSN: encrypted key data - hexdump(len=56): 15 7f 7a 3e 94 33 f6 d1 46 c1 d6 c9 57 39 77 91 fb 78 6e 7b 6a 28 fd f7 36 8d fe c1 13 3d 96 1a 22 fc 0b c0 64 23 e3 5a 72 da 95 6f 55 92 07 42 97 c8 d1 99 39 d0 6a 97
231117:112153 wpa_supplicant[20332]: WPA: Decrypt Key Data using AES-UNWRAP (KEK length 16)
231117:112153 wpa_supplicant[20332]: WPA: decrypted EAPOL-Key key data - hexdump(len=48): [REMOVED]
231117:112153 wpa_supplicant[20332]: wlan0: State: 4WAY_HANDSHAKE -> 4WAY_HANDSHAKE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: RX message 3 of 4-Way Handshake from 38:xx:xx:xx:ee:81 (ver=2)
231117:112153 wpa_supplicant[20332]: WPA: IE KeyData - hexdump(len=48): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00 dd 16 00 0f ac 01 01 00 92 0f ca f5 13 5d 88 f6 12 08 82 19 b1 22 48 34 dd 00
231117:112153 wpa_supplicant[20332]: WPA: RSN IE in EAPOL-Key - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112153 wpa_supplicant[20332]: WPA: GTK in EAPOL-Key - hexdump(len=24): [REMOVED]
231117:112153 wpa_supplicant[20332]: wlan0: WPA: No WPA/RSN IE for this AP known. Trying to get from scan results
231117:112153 wpa_supplicant[20332]: wlan0: WPA: clearing AP WPA IE
231117:112153 wpa_supplicant[20332]: WPA: set AP RSN IE - hexdump(len=22): 30 14 01 00 00 0f ac 04 01 00 00 0f ac 04 01 00 00 0f ac 02 0c 00
231117:112153 wpa_supplicant[20332]: wlan0: WPA: clearing AP RSNXE
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Found the current AP from updated scan results
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Sending EAPOL-Key 4/4
231117:112153 wpa_supplicant[20332]: WPA: Send EAPOL-Key frame to 38:xx:xx:xx:ee:81 ver=2 mic_len=16 key_mgmt=0x2
231117:112153 wpa_supplicant[20332]: WPA: EAPOL-Key MIC using HMAC-SHA1
231117:112153 wpa_supplicant[20332]: WPA: KCK - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: Derived Key MIC - hexdump(len=16): 1b 9a c7 35 a3 63 4d 27 a5 1f ac 5e 3f 02 fa 44
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Installing PTK to the driver
231117:112153 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=3 addr=0x7ad04c key_idx=0 set_tx=1 seq_len=6 key_len=16 key_flag=0x2c
231117:112153 wpa_supplicant[20332]: nl80211: NEW_KEY
231117:112153 wpa_supplicant[20332]: nl80211: KEY_DATA - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: nl80211: KEY_SEQ - hexdump(len=6): 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:    addr=38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]:    pairwise key
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portValid=1
231117:112153 wpa_supplicant[20332]: wlan0: State: 4WAY_HANDSHAKE -> GROUP_HANDSHAKE
231117:112153 wpa_supplicant[20332]: RSN: received GTK in pairwise handshake - hexdump(len=18): [REMOVED]
231117:112153 wpa_supplicant[20332]: WPA: Group Key - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Installing GTK to the driver (keyidx=1 tx=0 len=16)
231117:112153 wpa_supplicant[20332]: WPA: RSC - hexdump(len=6): 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=3 addr=0xa5f5b key_idx=1 set_tx=0 seq_len=6 key_len=16 key_flag=0x14
231117:112153 wpa_supplicant[20332]: nl80211: NEW_KEY
231117:112153 wpa_supplicant[20332]: nl80211: KEY_DATA - hexdump(len=16): [REMOVED]
231117:112153 wpa_supplicant[20332]: nl80211: KEY_SEQ - hexdump(len=6): 00 00 00 00 00 00
231117:112153 wpa_supplicant[20332]:    broadcast key
231117:112153 wpa_supplicant[20332]: wlan0: WPA: Key negotiation completed with 38:xx:xx:xx:ee:81 [PTK=CCMP GTK=CCMP]
231117:112153 wpa_supplicant[20332]: wlan0: Cancelling authentication timeout
231117:112153 wpa_supplicant[20332]: wlan0: State: GROUP_HANDSHAKE -> COMPLETED
231117:112153 wpa_supplicant[20332]: wlan0: Radio work 'connect'@0x7c3f90 done in 2.967559 seconds
231117:112153 wpa_supplicant[20332]: wlan0: radio_work_free('connect'@0x7c3f90): num_active_works --> 0
231117:112153 wpa_supplicant[20332]: wlan0: CTRL-EVENT-CONNECTED - Connection to 38:xx:xx:xx:ee:81 completed [id=0 id_str= freq=5200]
231117:112153 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->1 (UP)
231117:112153 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=6 (IF_OPER_UP)
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - portValid=1
231117:112153 wpa_supplicant[20332]: EAPOL: External notification - EAP success=1
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state AUTHENTICATING
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state SUCCESS
231117:112153 wpa_supplicant[20332]: EAP: EAP entering state DISABLED
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state AUTHENTICATED
231117:112153 wpa_supplicant[20332]: EAPOL: Supplicant port status: Authorized
231117:112153 wpa_supplicant[20332]: nl80211: Set supplicant port authorized for 38:xx:xx:xx:ee:81
231117:112153 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state IDLE
231117:112153 wpa_supplicant[20332]: EAPOL authentication completed - result=SUCCESS
231117:112153 wpa_supplicant[20332]: nl80211: Set rekey offload
231117:112153 wpa_supplicant[20332]: EAPOL: EAP Session-Id not available
231117:112155 wpa_supplicant[20332]: EAPOL: startWhen --> 0
231117:112155 wpa_supplicant[20332]: EAPOL: disable timer tick
231117:112156 wpa_supplicant[20332]: wlan0: Control interface command 'SET_NETWORK [REMOVED]'
231117:112156 wpa_supplicant[20332]: CTRL_IFACE: SET_NETWORK id=0 name='priority'
231117:112156 wpa_supplicant[20332]: CTRL_IFACE: value - hexdump(len=2): [REMOVED]
231117:112229 wpa_supplicant[20332]: wlan0: Control interface command 'DISCONNECT'
231117:112229 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112229 wpa_supplicant[20332]: wlan0: Request to deauthenticate - bssid=38:xx:xx:xx:ee:81 pending_bssid=00:xx:xx:xx:00:00 reason=3 (DEAUTH_LEAVING) state=COMPLETED
231117:112229 wpa_supplicant[20332]: wpa_driver_nl80211_disconnect(reason_code=3)
231117:112229 wpa_supplicant[20332]: wlan0: Event DEAUTH (11) received
231117:112229 wpa_supplicant[20332]: wlan0: Deauthentication notification
231117:112229 wpa_supplicant[20332]: wlan0:  * reason 3 (DEAUTH_LEAVING) locally_generated=1
231117:112229 wpa_supplicant[20332]: Deauthentication frame IE(s) - hexdump(len=0): [NULL]
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-DISCONNECTED bssid=38:xx:xx:xx:ee:81 reason=3 locally_generated=1
231117:112229 wpa_supplicant[20332]: wlan0: Auto connect disabled: do not try to re-connect
231117:112229 wpa_supplicant[20332]: wlan0: Ignore connection failure indication since interface has been put into disconnected state
231117:112229 wpa_supplicant[20332]: wlan0: WPA: Clear old PMK and PTK
231117:112229 wpa_supplicant[20332]: wlan0: Disconnect event - remove keys
231117:112229 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=0 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112229 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112229 wpa_supplicant[20332]:    broadcast key
231117:112229 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=(nil) key_idx=1 set_tx=0 seq_len=0 key_len=0 key_flag=0x10
231117:112229 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112229 wpa_supplicant[20332]:    broadcast key
231117:112229 wpa_supplicant[20332]: wpa_driver_nl80211_set_key: ifindex=38 (wlan0) alg=0 addr=0x7ab3ec key_idx=0 set_tx=0 seq_len=0 key_len=0 key_flag=0x20
231117:112229 wpa_supplicant[20332]: nl80211: DEL_KEY
231117:112229 wpa_supplicant[20332]:    addr=38:xx:xx:xx:ee:81
231117:112229 wpa_supplicant[20332]:    pairwise key
231117:112229 wpa_supplicant[20332]: wlan0: State: COMPLETED -> DISCONNECTED
231117:112229 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 1->0 (DORMANT)
231117:112229 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112229 wpa_supplicant[20332]: EAPOL: SUPP_PAE entering state DISCONNECTED
231117:112229 wpa_supplicant[20332]: EAPOL: Supplicant port status: Unauthorized
231117:112229 wpa_supplicant[20332]: nl80211: Skip set_supp_port(unauthorized) while not associated
231117:112229 wpa_supplicant[20332]: EAPOL: SUPP_BE entering state INITIALIZE
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - EAP success=0
231117:112229 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> DISCONNECTED
231117:112229 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112229 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112229 wpa_supplicant[20332]: QM: Clear all active DSCP policies
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-DSCP-POLICY clear_all
231117:112229 wpa_supplicant[20332]: nl80211: Drv Event 48 (NL80211_CMD_DISCONNECT) received for wlan0
231117:112229 wpa_supplicant[20332]: nl80211: Ignore disconnect event triggered during reassociation
231117:112229 wpa_supplicant[20332]: nl80211: Drv Event 36 (NL80211_CMD_REG_CHANGE) received for wlan0
231117:112229 wpa_supplicant[20332]: nl80211: Regulatory domain change
231117:112229 wpa_supplicant[20332]:  * initiator=0
231117:112229 wpa_supplicant[20332]:  * type=1
231117:112229 wpa_supplicant[20332]: wlan0: Event CHANNEL_LIST_CHANGED (27) received
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-REGDOM-CHANGE init=CORE type=WORLD
231117:112229 wpa_supplicant[20332]: wlan0: Updating hw mode
231117:112229 wpa_supplicant[20332]: nl80211: Regulatory information - country=IT (DFS-ETSI)
231117:112229 wpa_supplicant[20332]: nl80211: 2402-2482 @ 40 MHz 20 mBm
231117:112229 wpa_supplicant[20332]: nl80211: 5170-5250 @ 80 MHz 20 mBm
231117:112229 wpa_supplicant[20332]: nl80211: 5250-5330 @ 80 MHz 20 mBm (DFS)
231117:112229 wpa_supplicant[20332]: nl80211: 5490-5710 @ 160 MHz 27 mBm (DFS)
231117:112229 wpa_supplicant[20332]: nl80211: 57000-66000 @ 2160 MHz 40 mBm
231117:112229 wpa_supplicant[20332]: nl80211: Added 802.11b mode based on 802.11g information
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11g: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11a: 5180 5200 5220 5240 5260[NO_IR][RADAR] 5280[NO_IR][RADAR] 5300[NO_IR][RADAR] 5320[NO_IR][RADAR] 5500[NO_IR][RADAR] 5520[NO_IR][RADAR] 5540[NO_IR][RADAR] 5560[NO_IR][RADAR] 5580[NO_IR][RADAR]
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11b: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112229 wpa_supplicant[20332]: nl80211: Drv Event 36 (NL80211_CMD_REG_CHANGE) received for wlan0
231117:112229 wpa_supplicant[20332]: nl80211: Regulatory domain change
231117:112229 wpa_supplicant[20332]:  * initiator=1
231117:112229 wpa_supplicant[20332]:  * type=0
231117:112229 wpa_supplicant[20332]:  * alpha2=IT
231117:112229 wpa_supplicant[20332]: wlan0: Event CHANNEL_LIST_CHANGED (27) received
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-REGDOM-CHANGE init=USER type=COUNTRY alpha2=IT
231117:112229 wpa_supplicant[20332]: wlan0: Updating hw mode
231117:112229 wpa_supplicant[20332]: nl80211: Regulatory information - country=IT (DFS-ETSI)
231117:112229 wpa_supplicant[20332]: nl80211: 2402-2482 @ 40 MHz 20 mBm
231117:112229 wpa_supplicant[20332]: nl80211: 5170-5250 @ 80 MHz 20 mBm
231117:112229 wpa_supplicant[20332]: nl80211: 5250-5330 @ 80 MHz 20 mBm (DFS)
231117:112229 wpa_supplicant[20332]: nl80211: 5490-5710 @ 160 MHz 27 mBm (DFS)
231117:112229 wpa_supplicant[20332]: nl80211: 57000-66000 @ 2160 MHz 40 mBm
231117:112229 wpa_supplicant[20332]: nl80211: Added 802.11b mode based on 802.11g information
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11g: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11a: 5180 5200 5220 5240 5260[NO_IR][RADAR] 5280[NO_IR][RADAR] 5300[NO_IR][RADAR] 5320[NO_IR][RADAR] 5500[NO_IR][RADAR] 5520[NO_IR][RADAR] 5540[NO_IR][RADAR] 5560[NO_IR][RADAR] 5580[NO_IR][RADAR]
231117:112229 wpa_supplicant[20332]: nl80211: Mode IEEE 802.11b: 2412 2417 2422 2427 2432 2437 2442 2447 2452 2457 2462 2467 2472 2484[DISABLED]
231117:112229 wpa_supplicant[20332]: CTRL_IFACE monitor detached /tmp/wpa_ctrl_1633-44\x00
231117:112229 wpa_supplicant[20332]: wlan0: Removing interface wlan0
231117:112229 wpa_supplicant[20332]: nl80211: Getting wowlan status
231117:112229 wpa_supplicant[20332]: nl80211: wowlan is disabled
231117:112229 wpa_supplicant[20332]: wlan0: Request to deauthenticate - bssid=00:xx:xx:xx:00:00 pending_bssid=00:xx:xx:xx:00:00 reason=3 (DEAUTH_LEAVING) state=DISCONNECTED
231117:112229 wpa_supplicant[20332]: wlan0: State: DISCONNECTED -> DISCONNECTED
231117:112229 wpa_supplicant[20332]: nl80211: Set wlan0 operstate 0->0 (DORMANT)
231117:112229 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=-1 (no change), operstate=5 (IF_OPER_DORMANT)
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portEnabled=0
231117:112229 wpa_supplicant[20332]: EAPOL: External notification - portValid=0
231117:112229 wpa_supplicant[20332]: QM: Clear all active DSCP policies
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-DSCP-POLICY clear_all
231117:112229 wpa_supplicant[20332]: wlan0: WPA: Clear old PMK and PTK
231117:112229 wpa_supplicant[20332]: wlan0: Cancelling delayed sched scan
231117:112229 wpa_supplicant[20332]: wlan0: Cancelling scan request
231117:112229 wpa_supplicant[20332]: wlan0: Cancelling authentication timeout
231117:112229 wpa_supplicant[20332]: QM: Clear all active DSCP policies
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-DSCP-POLICY clear_all
231117:112229 wpa_supplicant[20332]: Remove interface wlan0 from radio phy0
231117:112229 wpa_supplicant[20332]: Remove radio phy0
231117:112229 wpa_supplicant[20332]: nl80211: deinit ifname=wlan0 disabled_11b_rates=0
231117:112229 wpa_supplicant[20332]: nl80211: Remove monitor interface: refcount=0
231117:112229 wpa_supplicant[20332]: netlink: Operstate: ifindex=38 linkmode=0 (kernel-control), operstate=6 (IF_OPER_UP)
231117:112229 wpa_supplicant[20332]: nl80211: Set mode ifindex 38 iftype 2 (STATION)
231117:112229 wpa_supplicant[20332]: nl80211: Unsubscribe mgmt frames handle 0x88f24279 (mode change)
231117:112229 wpa_supplicant[20332]: wlan0: CTRL-EVENT-TERMINATING 
